Date Generated

**Aug 16, 2022**

Call Order

**001**

Project ID

**E100203**

Amendments

**0**

Counties

**Dona Ana**

Highway Number

Time Remaining

Add to calendar

Days

**34**

Hours

**21**

Description

**Roadway Reconstruction, Lighting, ITS**

Items

Favorite items only

Edit favorites

Export

| **Line** | **Item** | **Description** | **Unit** | **Quantity** | **Price** | |
| --- | --- | --- | --- | --- | --- | --- |
| Section 0001: ROADWAY | | | | | | |
| 0010 | 107000 | ENVIRONMENTAL COMMITMENTS | LS | 1 |  |  |
| 0020 | 201000 | CLEARING AND GRUBBING | LS | 1 |  |  |
| 0030 | 203000 | UNCLASSIFIED EXCAVATION | C.Y. | 149000 |  |  |
| 0040 | 203100 | BORROW | C.Y. | 95000 |  |  |
| 0050 | 203211 | UNSTABLE SUBGRADE STABILIZATION | S.Y. | 69800 |  |  |
| 0060 | 206000 | UNSUITABLE MATERIAL EXCAVATION | C.Y. | 4700 |  |  |
| 0070 | 207000 | SUBGRADE PREPARATION | S.Y. | 464400 |  |  |
| 0080 | 213000 | OBLITERATING OLD ROAD | MILE | 0.34 |  |  |
| 0090 | 303000 | BASE COURSE | TON | 135270 |  |  |
| 0100 | 403715 | RUBBERIZED OPEN-GRADED FRICTION COURSE COMPLETE | TON | 7600 |  |  |
| 0110 | 405000 | DETOUR PAVEMENT CONSTRUCTION | S.Y. | 11000 |  |  |
| 0120 | 407000 | ASPHALT MATERIAL FOR TACK COAT | TON | 400 |  |  |
| 0130 | 408100 | PRIME COAT MATERIAL | TON | 808 |  |  |
| 0140 | 423283 | HMA SP-IV COMPLETE | TON | 166440 |  |  |
| 0150 | 502030 | DRILLED SHAFT FOUNDATION 30" DIAMETER | L.F. | 75 |  |  |
| 0160 | 511000 | STRUCTURAL CONCRETE, CLASS A | C.Y. | 620 |  |  |
| 0170 | 511030 | STRUCTURAL CONCRETE, CLASS AA | C.Y. | 1400 |  |  |
| 0180 | 531001 | PERMANENT ANTI-GRAFFITI PROTECTIVE COATING | S.F. | 282810 |  |  |
| 0190 | 540060 | REINFORCING BARS GRADE 60 | LB | 444220 |  |  |
| 0200 | 541200 | STRUCTURAL STEEL FOR MISCELLANEOUS STRUCTURES | LB | 31020 |  |  |
| 0210 | 570018 | 18" CULVERT PIPE | L.F. | 356 |  |  |
| 0220 | 570024 | 24" CULVERT PIPE | L.F. | 1512 |  |  |
| 0230 | 570030 | 30" CULVERT PIPE | L.F. | 978 |  |  |
| 0240 | 570036 | 36" CULVERT PIPE | L.F. | 430 |  |  |
| 0250 | 570037 | 36" CULVERT PIPE END SECTION | EACH | 2 |  |  |
| 0260 | 570042 | 42" CULVERT PIPE | L.F. | 182 |  |  |
| 0270 | 570048 | 48" CULVERT PIPE | L.F. | 462 |  |  |
| 0280 | 570049 | 48" CULVERT PIPE END SECTION | EACH | 1 |  |  |
| 0290 | 570054 | 54" CULVERT PIPE | L.F. | 152 |  |  |
| 0300 | 570084 | 84" CULVERT PIPE | L.F. | 50 |  |  |
| 0310 | 570170 | 64"SX43"R (NOMINAL) CULVERT PIPE ARCH | L.F. | 400 |  |  |
| 0320 | 570174 | 71"SX47"R (NOMINAL) CULVERT PIPE ARCH | L.F. | 410 |  |  |
| 0330 | 570437 | 24" STORM DRAIN CULVERT PIPE | L.F. | 688 |  |  |
| 0340 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| 0350 | 601110 | REMOVAL OF SURFACING | S.Y. | 207300 |  |  |
| 0360 | 602000 | RIPRAP CLASS A | C.Y. | 525 |  |  |
| 0370 | 603100 | TEMPORARY SOIL STABILANT | ACRE | 44 |  |  |
| 0380 | 603250 | DROP INLET PROTECTION TYPE I | EACH | 19 |  |  |
| 0390 | 603262 | COMPOSTED MULCH SOCKS | L.F. | 8630 |  |  |
| 0400 | 603281 | SWPPP PLAN PREPARATION AND MAINTENANCE | LS | 1 |  |  |
| 0410 | 606001 | SINGLE FACE W-BEAM GUARDRAIL | L.F. | 4475 |  |  |
| 0420 | 606051 | END TREATMENT TL-3 END TERMINAL | EACH | 10 |  |  |
| 0430 | 606053 | END TREATMENT W-BEAM END ANCHOR | EACH | 3 |  |  |
| 0440 | 606062 | TRANSITION METAL BARRIER TO RIGID BARRIER | EACH | 7 |  |  |
| 0450 | 606542 | CONCRETE WALL BARRIER 42" | L.F. | 33790 |  |  |
| 0460 | 606590 | CONCRETE WALL BARRIER (MODIFIED) | L.F. | 1390 |  |  |
| 0470 | 606710 | TCWB RETAINED BY THE CONTRACTOR (20') | L.F. | 2690 |  |  |
| 0480 | 606719 | RESETTING OF TCWB (20') | L.F. | 7500 |  |  |
| 0490 | 607012 | GAME FENCE | L.F. | 86320 |  |  |
| 0500 | 607015 | BRACES/CORNER POSTS | EACH | 187 |  |  |
| 0510 | 607314 | STANDARD GATE, 14' | EACH | 2 |  |  |
| 0520 | 607506 | PIPE GATE 6' | EACH | 2 |  |  |
| 0530 | 608004 | CONCRETE SIDEWALK 4" | S.Y. | 600 |  |  |
| 0540 | 608204 | CONCRETE MEDIAN PAVEMENT 4" | S.Y. | 1700 |  |  |
| 0550 | 609324 | CONCRETE SLOPED CURB AND GUTTER 6" X 24" | L.F. | 13800 |  |  |
| 0560 | 609424 | CONCRETE VERTICAL CURB AND GUTTER TYPE B 6" X 24" | L.F. | 1900 |  |  |
| 0570 | 609478 | CONCRETE VERTICAL CURB AND GUTTER TYPE D 6" X 18" | L.F. | 1530 |  |  |
| 0580 | 610000 | CATTLE GUARD | L.F. | 64 |  |  |
| 0590 | 617000 | VIBRATION MONITORING | LS | 1 |  |  |
| 0600 | 617003 | VIDEO RECORDING | LS | 1 |  |  |
| 0610 | 618000 | TRAFFIC CONTROL MANAGEMENT | LS | 1 |  |  |
| 0620 | 618011 | PUBLIC AWARENESS | LS | 1 |  |  |
| 0630 | 621000 | MOBILIZATION | LS | 1 |  |  |
| 0640 | 623021 | MEDIAN DROP INLET TYPE II (URBAN) | EACH | 1 |  |  |
| 0650 | 623301 | CURB DROP INLET TYPE I-A, 0' TO 4' | EACH | 1 |  |  |
| 0660 | 623313 | CURB DROP INLET TYPE III-B, 0' TO 4' | EACH | 1 |  |  |
| 0670 | 623331 | CURB DROP INLET TYPE I-B, OVER 4' | EACH | 3 |  |  |
| 0680 | 623332 | CURB DROP INLET TYPE II-B, OVER 4' | EACH | 2 |  |  |
| 0690 | 623401 | DROP INLET 4'X4'(TYPE I) H=4'-0" | EACH | 12 |  |  |
| 0700 | 623402 | DROP INLET 4'X4' (TYPE II) H=4'-0" | EACH | 3 |  |  |
| 0710 | 623403 | DROP INLET 4'X4' (TYPE III) H=4'-0" | EACH | 1 |  |  |
| 0720 | 623407 | DROP INLET 4'X4' (TYPE I) H=6'-1" TO 8'-0" | EACH | 2 |  |  |
| 0730 | 623600 | JUNCTION BOX | EACH | 6 |  |  |
| 0740 | 631000 | RUMBLE STRIPS | L.F. | 82310 |  |  |
| 0750 | 632000 | CLASS A SEEDING | ACRE | 39 |  |  |
| 0760 | 632020 | CLASS C SEEDING | ACRE | 4 |  |  |
| 0770 | 662000 | MANHOLE TYPE C-4' DIAMETER 0' TO 6' DEPTH | EACH | 1 |  |  |
| 0780 | 662400 | MANHOLE ADJUSTMENT | EACH | 1 |  |  |
| 0790 | 701000 | PANEL SIGNS | S.F. | 1300 |  |  |
| 0800 | 701030 | REMOVE AND RESET PANEL SIGN | EACH | 6 |  |  |
| 0810 | 701100 | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS | L.F. | 2350 |  |  |
| 0820 | 702000 | CONSTRUCTION SIGNING | S.F. | 850 |  |  |
| 0830 | 702100 | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING | L.F. | 2300 |  |  |
| 0840 | 702101 | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING | EACH | 9 |  |  |
| 0850 | 702110 | PORTABLE SIGN SUPPORT | EACH | 1 |  |  |
| 0860 | 702238 | BARRICADE, TYPE III-8' | EACH | 14 |  |  |
| 0870 | 702525 | CHANNELIZATION DEVICES TYPE DRUM | EACH | 1115 |  |  |
| 0880 | 702610 | PORTABLE CHANGEABLE MESSAGE SIGN | EACH | 5 |  |  |
| 0890 | 702850 | LAW ENFORCEMENT IN CONSTRUCTION ZONE | ALOW | 1 | $25,000.00 |  |
| 0900 | 704000 | RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 202770 |  |  |
| 0910 | 704005 | RETROREFLECTORIZED PAINTED MARKINGS 24" | L.F. | 30 |  |  |
| 0920 | 704099 | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 436230 |  |  |
| 0930 | 704704 | HOT THERMOPLASTIC PAVEMENT MARKING 24" | L.F. | 110 |  |  |
| 0940 | 704718 | HOT THERMOPLASTIC PAVEMENT MARKING LEFT ARROW | EACH | 22 |  |  |
| 0950 | 704720 | HOT THERMOPLASTIC PAVEMENT MARKING WORD (ONLY) | EACH | 10 |  |  |
| 0960 | 704731 | HOT THERMOPLASTIC MARKING LANE SYMBOL (BIKEWAY) | EACH | 1 |  |  |
| 0970 | 707540 | TYPE V STANDARD, 40' | EACH | 10 |  |  |
| 0980 | 709020 | RIGID ELECTRICAL CONDUIT 2" (DIA.) | L.F. | 2085 |  |  |
| 0990 | 710000 | ELECTRICAL PULL BOX (STANDARD) | EACH | 4 |  |  |
| 1000 | 711102 | SINGLE CONDUCTOR 2 | L.F. | 4150 |  |  |
| 1010 | 716701 | LED ROADWAY LUMINAIRE | EACH | 10 |  |  |
| 1020 | 720050 | PERMANENT VEHICULAR IMPACT ATTENUATOR UNIT | EACH | 11 |  |  |
| 1030 | 720060 | VEHICULAR IMPACT ATTENUATOR UNIT-WORK ZONES | EACH | 10 |  |  |
| 1040 | 720110 | REMOVE/RESET IMPACT ATTENUATOR UNIT | EACH | 28 |  |  |
| 1050 | 721000 | REMOVAL OF PAVEMENT MARKING | L.F. | 263600 |  |  |
| 1060 | 721101 | REMOVAL OF PAVEMENT MARKING SYMBOL | EACH | 1 |  |  |
| 1070 | 750034 | MULTI-DUCT CONDUIT 4" (6-WAY) | L.F. | 42800 |  |  |
| 1080 | 750060 | ITS PULLBOX (33"X24"X24") | EACH | 34 |  |  |
| 1090 | 750080 | ITS MANHOLE (48"X48"X48") | EACH | 8 |  |  |
| 1100 | 801000 | CONSTRUCTION STAKING BY THE CONTRACTOR | LS | 1 |  |  |
| 1110 | 802000 | POST CONSTRUCTION PLANS | LS | 1 | $5,250.00 |  |
| 1120 | 803000 | SCHEDULE SOFTWARE | LS | 1 |  |  |
| 1130 | 803010 | CPM TRAINING | LS | 1 |  |  |
| 1140 | 803020 | CPM HARDWARE/EQUIPMENT | LS | 1 |  |  |
| Showing **114** items | | | | | | |