Letting of Dec 16, 2022: 1 of 2

**2101351**

Date Generated

**Nov 14, 2022**

Call Order

**001**

Project ID

**2101351**

Amendments

**0**

Counties

**Curry**

Highway Number

Time Remaining

Add to calendar

Days

**25**

Hours

**2**

Description

**Roadway Reconstruction, Signalization, Lighting**

Items

Favorite items only

Edit favorites

Export

| **Line** | **Item** | **Description** | **Unit** | **Quantity** | **Price** | |
| --- | --- | --- | --- | --- | --- | --- |
| Section 0001: ROADWAY | | | | | | |
| 0010 | 201000 | CLEARING AND GRUBBING | LS | 1 |  |  |
| 0020 | 203000 | UNCLASSIFIED EXCAVATION | C.Y. | 55000 |  |  |
| 0030 | 203200 | UNSUITABLE MATERIAL EXCAVATION | C.Y. | 7500 |  |  |
| 0040 | 203211 | UNSTABLE SUBGRADE STABILIZATION | S.Y. | 1180 |  |  |
| 0050 | 206000 | UNSUITABLE MATERIAL EXCAVATION | C.Y. | 750 |  |  |
| 0060 | 207000 | SUBGRADE PREPARATION | S.Y. | 11800 |  |  |
| 0070 | 210002 | MAJOR STRUCTURE EXCAVATION | C.Y. | 390 |  |  |
| 0080 | 210003 | MAJOR STRUCTURE BACKFILL | C.Y. | 410 |  |  |
| 0090 | 303000 | BASE COURSE | TON | 14320 |  |  |
| 0100 | 306102 | LIME TREATED SUBGRADE 12" | S.Y. | 31000 |  |  |
| 0110 | 402460 | HYDRATED LIME | TON | 800 |  |  |
| 0120 | 405000 | DETOUR PAVEMENT CONSTRUCTION | S.Y. | 6800 |  |  |
| 0130 | 407000 | ASPHALT MATERIAL FOR TACK COAT | TON | 9 |  |  |
| 0140 | 408100 | PRIME COAT MATERIAL | TON | 35 |  |  |
| 0150 | 416103 | MINOR PAVING TYPE I, HMA SP-III | TON | 1100 |  |  |
| 0160 | 416104 | MINOR PAVING TYPE I, HMA SP-IV | TON | 4100 |  |  |
| 0170 | 416207 | MINOR PAVING TYPE II, HMA SP-IV | S.Y. | 400 |  |  |
| 0180 | 417100 | ASPHALT CURB | L.F. | 1840 |  |  |
| 0190 | 450060 | CONCRETE PAVEMENT-6" | S.Y. | 4960 |  |  |
| 0200 | 450100 | CONCRETE PAVEMENT-10" | S.Y. | 24400 |  |  |
| 0210 | 452000 | SEALING CONCRETE PAVEMENT JOINTS | L.F. | 41480 |  |  |
| 0220 | 455100 | DIAMOND GROOVING OF PCCP | S.Y. | 24400 |  |  |
| 0230 | 502030 | DRILLED SHAFT FOUNDATION 30" DIAMETER | L.F. | 300 |  |  |
| 0240 | 502036 | DRILLED SHAFT FOUNDATION 36" DIAMETER | L.F. | 40 |  |  |
| 0250 | 502042 | DRILLED SHAFT FOUNDATION 42" DIAMETER | L.F. | 100 |  |  |
| 0260 | 511000 | STRUCTURAL CONCRETE, CLASS A | C.Y. | 5 |  |  |
| 0270 | 511200 | STRUCTURAL CONCRETE, CLASS A-4" | S.Y. | 6475 |  |  |
| 0280 | 515000 | REINF.CONCRETE FOR MINOR STRUCTURES | C.Y. | 190 |  |  |
| 0290 | 540060 | REINFORCING BARS GRADE 60 | LB | 17250 |  |  |
| 0300 | 570437 | 24" STORM DRAIN CULVERT PIPE | L.F. | 2070 |  |  |
| 0310 | 570449 | 30" STORM DRAIN CULVERT PIPE | L.F. | 330 |  |  |
| 0320 | 570461 | 36" STORM DRAIN CULVERT PIPE | L.F. | 590 |  |  |
| 0330 | 570467 | 42" STORM DRAIN CULVERT PIPE | L.F. | 220 |  |  |
| 0340 | 570473 | 48" STORM DRAIN CULVERT PIPE | L.F. | 230 |  |  |
| 0350 | 570486 | 60" STORM DRAIN CULVERT PIPE | L.F. | 50 |  |  |
| 0360 | 570500 | 72" STORM DRAIN CULVERT PIPE | L.F. | 11410 |  |  |
| 0370 | 570630 | 43"SX26"R STORM DRAIN CPA | L.F. | 870 |  |  |
| 0380 | 570868 | 18" CORRUGATED PIPE SLOTTED DRAIN | L.F. | 340 |  |  |
| 0390 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| 0400 | 601110 | REMOVAL OF SURFACING | S.Y. | 44540 |  |  |
| 0410 | 601300 | DEMOLITION | LS | 1 |  |  |
| 0420 | 601995 | AC-ABATEMENT | L.F. | 400 |  |  |
| 0430 | 602010 | RIPRAP CLASS B | C.Y. | 105 |  |  |
| 0440 | 603100 | TEMPORARY SOIL STABILANT | ACRE | 3 |  |  |
| 0450 | 603262 | COMPOSTED MULCH SOCKS | L.F. | 7240 |  |  |
| 0460 | 603281 | SWPPP PLAN PREPARATION AND MAINTENANCE | LS | 1 |  |  |
| 0470 | 606598 | TCWB RETAINED BY THE CONTRACTOR | L.F. | 6180 |  |  |
| 0480 | 606599 | RESETTING OF TCWB | L.F. | 18600 |  |  |
| 0490 | 607024 | CHAIN LINK FENCE 4' | L.F. | 190 |  |  |
| 0500 | 607046 | CHAIN LINK FENCE SECURITY FENCE 6' | L.F. | 320 |  |  |
| 0510 | 607079 | PEDESTRIAN/BICYCLE RAILING | L.F. | 560 |  |  |
| 0520 | 607199 | REMOVE AND REBUILD FENCE | L.F. | 500 |  |  |
| 0530 | 607408 | CHAIN LINK GATE, 8' (SPAN) | EACH | 2 |  |  |
| 0540 | 607410 | CHAIN LINK GATE, 10' (SPAN) | EACH | 4 |  |  |
| 0550 | 608004 | CONCRETE SIDEWALK 4" | S.Y. | 4120 |  |  |
| 0560 | 608106 | DRIVE PAD 6" | S.Y. | 1870 |  |  |
| 0570 | 608404 | CONCRETE MEDIAN PAVEMENT 4" (COLORED AND PATTERNED) | S.Y. | 760 |  |  |
| 0580 | 609424 | CONCRETE VERTICAL CURB AND GUTTER TYPE B 6" X 24" | L.F. | 9090 |  |  |
| 0590 | 609478 | CONCRETE VERTICAL CURB AND GUTTER TYPE D 6" X 18" | L.F. | 6120 |  |  |
| 0600 | 609636 | CONCRETE VALLEY GUTTER 6" X 36" | L.F. | 650 |  |  |
| 0610 | 609706 | CONCRETE LAYDOWN CURB 6" | L.F. | 1930 |  |  |
| 0620 | 617000 | VIBRATION MONITORING | LS | 1 |  |  |
| 0630 | 617003 | VIDEO RECORDING | LS | 1 |  |  |
| 0640 | 617004 | VIBRATION RISK SURVEY | LS | 1 |  |  |
| 0650 | 618000 | TRAFFIC CONTROL MANAGEMENT | LS | 1 |  |  |
| 0660 | 618011 | PUBLIC AWARENESS | LS | 1 | $50,000.00 |  |
| 0670 | 621000 | MOBILIZATION | LS | 1 |  |  |
| 0680 | 623003 | MEDIAN DROP INLET, TYPE I, 3' TO 6' | EACH | 4 |  |  |
| 0690 | 623006 | MEDIAN DROP INLET, TYPE I, 6' TO 8' | EACH | 6 |  |  |
| 0700 | 623008 | MEDIAN DROP INLET, TYPE I, 8' TO 10' | EACH | 1 |  |  |
| 0710 | 623312 | CURB DROP INLET TYPE II-B, 0' TO 4' | EACH | 1 |  |  |
| 0720 | 623331 | CURB DROP INLET TYPE I-B, OVER 4' | EACH | 37 |  |  |
| 0730 | 623332 | CURB DROP INLET TYPE II-B, OVER 4' | EACH | 32 |  |  |
| 0740 | 623333 | CURB DROP INLET TYPE III-B, OVER 4' | EACH | 9 |  |  |
| 0750 | 623334 | CURB DROP INLET TYPE IV-B, OVER 4' | EACH | 8 |  |  |
| 0760 | 632000 | CLASS A SEEDING | ACRE | 2 |  |  |
| 0770 | 662010 | MANHOLE TYPE C-6' DIAMETER 0' TO 6' DEPTH | EACH | 10 |  |  |
| 0780 | 662022 | MANHOLE TYPE C-6' DIAMETER OVER 6' TO 10' DEPTH | EACH | 3 |  |  |
| 0790 | 662040 | MANHOLE TYPE C-8' DIAMETER 0' TO 6' DEPTH | EACH | 3 |  |  |
| 0800 | 662042 | MANHOLE TYPE C-8' DIAMETER OVER 6' TO 10' DEPTH | EACH | 10 |  |  |
| 0810 | 662044 | MANHOLE TYPE C-8' DIAMETER OVER 10' TO 14' DEPTH | EACH | 19 |  |  |
| 0820 | 662100 | SPECIAL MANHOLE | EACH | 21 |  |  |
| 0830 | 663049 | PRECONSTRUCTION UTILITY SURVEY | LS | 1 |  |  |
| 0840 | 663206 | WATER SYSTEM | LS | 1 |  |  |
| 0850 | 663207 | SEWER SYSTEM | LS | 1 |  |  |
| 0860 | 663820 | PUMP STATION | LS | 1 |  |  |
| 0870 | 663855 | ADJUST VALVE BOX TO GRADE | EACH | 13 |  |  |
| 0880 | 663865 | ADJUST WATER METER TO GRADE | EACH | 8 |  |  |
| 0890 | 701000 | PANEL SIGNS | S.F. | 510 |  |  |
| 0900 | 701100 | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS | L.F. | 730 |  |  |
| 0910 | 702000 | CONSTRUCTION SIGNING | S.F. | 2440 |  |  |
| 0920 | 702100 | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING | L.F. | 4350 |  |  |
| 0930 | 702101 | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING | EACH | 6 |  |  |
| 0940 | 702110 | PORTABLE SIGN SUPPORT | EACH | 43 |  |  |
| 0950 | 702238 | BARRICADE, TYPE III-8' | EACH | 28 |  |  |
| 0960 | 702320 | VERTICAL PANEL, TYPE BACK TO BACK | EACH | 150 |  |  |
| 0970 | 702525 | CHANNELIZATION DEVICES TYPE DRUM | EACH | 230 |  |  |
| 0980 | 702600 | SEQUENTIAL ARROW DISPLAY | EACH | 5 |  |  |
| 0990 | 702610 | PORTABLE CHANGEABLE MESSAGE SIGN | EACH | 8 |  |  |
| 1000 | 702700 | TEMPORARY SIGNAL SPAN | LS | 1 |  |  |
| 1010 | 702850 | LAW ENFORCEMENT IN CONSTRUCTION ZONE | ALOW | 1 | $50,000.00 |  |
| 1020 | 704099 | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 34310 |  |  |
| 1030 | 704100 | REMOVABLE MARKING TAPE 4" | L.F. | 39210 |  |  |
| 1040 | 704104 | REMOVABLE MARKING TAPE 12" | L.F. | 1680 |  |  |
| 1050 | 704105 | REMOVABLE MARKING TAPE 24" | L.F. | 1030 |  |  |
| 1060 | 704700 | HOT THERMOPLASTIC PAVEMENT MARKINGS 4" | L.F. | 15700 |  |  |
| 1070 | 704702 | HOT THERMOPLASTIC PAVEMENT MARKINGS 8" | L.F. | 5600 |  |  |
| 1080 | 704704 | HOT THERMOPLASTIC PAVEMENT MARKING 24" | L.F. | 1300 |  |  |
| 1090 | 704717 | HOT THERMOPLASTIC PAVEMENT MARKING RIGHT ARROW | EACH | 8 |  |  |
| 1100 | 704718 | HOT THERMOPLASTIC PAVEMENT MARKING LEFT ARROW | EACH | 12 |  |  |
| 1110 | 704720 | HOT THERMOPLASTIC PAVEMENT MARKING WORD (ONLY) | EACH | 7 |  |  |
| 1120 | 705000 | SIGNAL/LIGHTING SYSTEM START-UP COSTS | ALOW | 1 | $13,600.00 |  |
| 1130 | 706000 | SERVICE POLE (SIGNAL) | EACH | 2 |  |  |
| 1140 | 706230 | METER PEDESTAL (COMBINATION) | EACH | 2 |  |  |
| 1150 | 706350 | POWER SERVICE INSTALLATION | LS | 1 | $42,000.00 |  |
| 1160 | 707004 | TYPE I STANDARD, 4' | EACH | 9 |  |  |
| 1170 | 707330 | TYPE III STANDARD, 30' ARM | EACH | 1 |  |  |
| 1180 | 707335 | TYPE III STANDARD, 35' ARM | EACH | 1 |  |  |
| 1190 | 707340 | TYPE III STANDARD, 40' ARM | EACH | 6 |  |  |
| 1200 | 709020 | RIGID ELECTRICAL CONDUIT 2" (DIA.) | L.F. | 9450 |  |  |
| 1210 | 709030 | RIGID ELECTRICAL CONDUIT 3" (DIA.) | L.F. | 1300 |  |  |
| 1220 | 710000 | ELECTRICAL PULL BOX (STANDARD) | EACH | 15 |  |  |
| 1230 | 710010 | ELECTRICAL PULL BOX (LARGE) | EACH | 13 |  |  |
| 1240 | 710400 | TRAFFIC SIGNAL MANHOLE | EACH | 2 |  |  |
| 1250 | 711005 | MULTI CONDUCTOR CABLE 5 | L.F. | 5000 |  |  |
| 1260 | 711007 | MULTI CONDUCTOR CABLE 7 | L.F. | 400 |  |  |
| 1270 | 711020 | MULTI CONDUCTOR CABLE 20 | L.F. | 3100 |  |  |
| 1280 | 711102 | SINGLE CONDUCTOR 2 | L.F. | 300 |  |  |
| 1290 | 711106 | SINGLE CONDUCTOR 6 | L.F. | 3700 |  |  |
| 1300 | 712031 | 3 SECTION TRAFFIC SIGNAL ASSEMBLY (LED) | EACH | 17 |  |  |
| 1310 | 712051 | 5 SECTION TRAFFIC SIGNAL ASSEMBLY (LED) | EACH | 14 |  |  |
| 1320 | 712202 | PEDESTRIAN COUNTDOWN SIGNAL (LED) | EACH | 16 |  |  |
| 1330 | 712330 | 3 SECTION BACKPLATE | EACH | 8 |  |  |
| 1340 | 712350 | 5 SECTION BACKPLATE | EACH | 7 |  |  |
| 1350 | 713025 | ACCESSIBLE PEDESTRIAN SIGNAL PUSH BUTTON STATION | EACH | 16 |  |  |
| 1360 | 713807 | VIDEO CABLE | L.F. | 1800 |  |  |
| 1370 | 713810 | VIDEO CAMERA | EACH | 10 |  |  |
| 1380 | 713825 | VIDEO HARDWARE SYSTEM | EACH | 2 |  |  |
| 1390 | 714000 | TRAFFIC ACTUATED CONTROLLER | EACH | 2 |  |  |
| 1400 | 714280 | 8 PHASE DOUBLE RING CONTROLLER CABINET | EACH | 2 |  |  |
| 1410 | 716000 | LIGHTING SYSTEM | LS | 1 | $374,000.00 |  |
| 1420 | 716301 | INTERNALLY ILLUMINATED SIGN | EACH | 8 |  |  |
| 1430 | 716701 | LED ROADWAY LUMINAIRE | EACH | 8 |  |  |
| 1440 | 720060 | VEHICULAR IMPACT ATTENUATOR UNIT-WORK ZONES | EACH | 4 |  |  |
| 1450 | 720110 | REMOVE/RESET IMPACT ATTENUATOR UNIT | EACH | 21 |  |  |
| 1460 | 721000 | REMOVAL OF PAVEMENT MARKING | L.F. | 63190 |  |  |
| 1470 | 801000 | CONSTRUCTION STAKING BY THE CONTRACTOR | LS | 1 |  |  |
| 1480 | 802000 | POST CONSTRUCTION PLANS | LS | 1 | $31,500.00 |  |
| 1490 | 803000 | SCHEDULE SOFTWARE | LS | 1 |  |  |
| 1500 | 803020 | CPM HARDWARE/EQUIPMENT | LS | 1 |  |  |

Letting of Dec 16, 2022: 2 of 2

**4100701**

Date Generated

**Nov 14, 2022**

Call Order

**002**

Project ID

**4100701**

Amendments

**0**

Counties

**Colfax**

Highway Number

Time Remaining

Add to calendar

Days

**25**

Hours

**2**

Description

**Roadway Rehabilitation and Reconstruction, ITS**

Items

Favorite items only

Edit favorites

Export

| **Line** | **Item** | **Description** | **Unit** | **Quantity** | **Price** | |
| --- | --- | --- | --- | --- | --- | --- |
| Section 0001: ROADWAY | | | | | | |
| 0010 | 107000 | ENVIRONMENTAL COMMITMENTS | LS | 1 |  |  |
| 0020 | 201000 | CLEARING AND GRUBBING | LS | 1 |  |  |
| 0030 | 203000 | UNCLASSIFIED EXCAVATION | C.Y. | 26000 |  |  |
| 0040 | 203211 | UNSTABLE SUBGRADE STABILIZATION | S.Y. | 14600 |  |  |
| 0050 | 203301 | ROCK EXCAVATION | C.Y. | 6500 |  |  |
| 0060 | 206100 | SELECT BACKFILL MATERIAL | C.Y. | 270 |  |  |
| 0070 | 207000 | SUBGRADE PREPARATION | S.Y. | 52695 |  |  |
| 0080 | 210002 | MAJOR STRUCTURE EXCAVATION | C.Y. | 1790 |  |  |
| 0090 | 210003 | MAJOR STRUCTURE BACKFILL | C.Y. | 2390 |  |  |
| 0100 | 303000 | BASE COURSE | TON | 14125 |  |  |
| 0110 | 405000 | DETOUR PAVEMENT CONSTRUCTION | S.Y. | 3150 |  |  |
| 0120 | 407000 | ASPHALT MATERIAL FOR TACK COAT | TON | 30 |  |  |
| 0130 | 408100 | PRIME COAT MATERIAL | TON | 93 |  |  |
| 0140 | 414130 | COLD MILLING (ASPHALT) 3" | S.Y. | 55000 |  |  |
| 0150 | 416216 | MINOR PAVING TYPE II, WMA SP-III | S.Y. | 985 |  |  |
| 0160 | 424003 | WMA SP-III COMPLETE | TON | 20140 |  |  |
| 0170 | 511000 | STRUCTURAL CONCRETE, CLASS A | C.Y. | 800 |  |  |
| 0180 | 511030 | STRUCTURAL CONCRETE, CLASS AA | C.Y. | 340 |  |  |
| 0190 | 515000 | REINF.CONCRETE FOR MINOR STRUCTURES | C.Y. | 25 |  |  |
| 0200 | 540060 | REINFORCING BARS GRADE 60 | LB | 113810 |  |  |
| 0210 | 541200 | STRUCTURAL STEEL FOR MISCELLANEOUS STRUCTURES | LB | 110 |  |  |
| 0220 | 570024 | 24" CULVERT PIPE | L.F. | 240 |  |  |
| 0230 | 570025 | 24" CULVERT PIPE END SECTION | EACH | 18 |  |  |
| 0240 | 570030 | 30" CULVERT PIPE | L.F. | 260 |  |  |
| 0250 | 570031 | 30" CULVERT PIPE END SECTION | EACH | 14 |  |  |
| 0260 | 570036 | 36" CULVERT PIPE | L.F. | 150 |  |  |
| 0270 | 570037 | 36" CULVERT PIPE END SECTION | EACH | 6 |  |  |
| 0280 | 571263 | 11'2''S X 3'6''R STRUCTURAL PLATE PIPE ARCH | L.F. | 130 |  |  |
| 0290 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| 0300 | 602000 | RIPRAP CLASS A | C.Y. | 50 |  |  |
| 0310 | 602200 | GABIONS | C.Y. | 6860 |  |  |
| 0320 | 603050 | CLEAN WATER ACT COMPLIANCE WORK PLAN | ALOW | 1 | $10,000.00 |  |
| 0330 | 603100 | TEMPORARY SOIL STABILANT | ACRE | 10.8 |  |  |
| 0340 | 603221 | CHECK DAM TYPE II | L.F. | 160 |  |  |
| 0350 | 603262 | COMPOSTED MULCH SOCKS | L.F. | 6480 |  |  |
| 0360 | 603281 | SWPPP PLAN PREPARATION AND MAINTENANCE | LS | 1 |  |  |
| 0370 | 604001 | GEOTEXTILE CLASS 1 | S.Y. | 1985 |  |  |
| 0380 | 606001 | SINGLE FACE W-BEAM GUARDRAIL | L.F. | 8000 |  |  |
| 0390 | 606051 | END TREATMENT TL-3 END TERMINAL | EACH | 4 |  |  |
| 0400 | 606052 | END TREATMENT TL-2 END TERMINAL | EACH | 16 |  |  |
| 0410 | 606053 | END TREATMENT W-BEAM END ANCHOR | EACH | 16 |  |  |
| 0420 | 606055 | END TREATMENT DRIVEWAY END ANCHOR | EACH | 4 |  |  |
| 0430 | 606061 | DRAINAGE STRUCTURE PROTECTION SYSTEM | L.F. | 37.5 |  |  |
| 0440 | 606062 | TRANSITION METAL BARRIER TO RIGID BARRIER | EACH | 4 |  |  |
| 0450 | 606542 | CONCRETE WALL BARRIER 42" | L.F. | 1930 |  |  |
| 0460 | 606598 | TCWB RETAINED BY THE CONTRACTOR | L.F. | 1440 |  |  |
| 0470 | 606599 | RESETTING OF TCWB | L.F. | 300 |  |  |
| 0480 | 609600 | CONCRETE VALLEY GUTTER SPECIAL DESIGN | L.F. | 100 |  |  |
| 0490 | 613000 | CLEANING CULVERTS AND DRAINAGE STRUCTURES | LS | 1 |  |  |
| 0500 | 618000 | TRAFFIC CONTROL MANAGEMENT | LS | 1 |  |  |
| 0510 | 618011 | PUBLIC AWARENESS | LS | 1 |  |  |
| 0520 | 621000 | MOBILIZATION | LS | 1 |  |  |
| 0530 | 622002 | FIELD LABORATORY, TYPE II | EACH | 1 |  |  |
| 0540 | 622100 | SUPPLEMENTAL FIELD LABORATORY | EACH | 1 |  |  |
| 0550 | 622110 | SUPPLEMENTAL HOT-MIX ASPHALT FIELD LABORATORY | EACH | 1 |  |  |
| 0560 | 622200 | FIELD OFFICE | EACH | 1 |  |  |
| 0570 | 623102 | MEDIAN DROP INLET TYPE II | EACH | 2 |  |  |
| 0580 | 623345 | CURB DROP INLET FOR CONCRETE WALL BARRIER | EACH | 1 |  |  |
| 0590 | 631000 | RUMBLE STRIPS | L.F. | 17970 |  |  |
| 0600 | 632000 | CLASS A SEEDING | ACRE | 3 |  |  |
| 0610 | 632020 | CLASS C SEEDING | ACRE | 6 |  |  |
| 0620 | 701000 | PANEL SIGNS | S.F. | 910 |  |  |
| 0630 | 701100 | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS | L.F. | 1905 |  |  |
| 0640 | 701112 | STEEL I-BEAM POST TYPE W6X12 | L.F. | 32 |  |  |
| 0650 | 701212 | BREAKAWAY BASE SYSTEM FOR STEEL I BEAM POST W6X12 | EACH | 2 |  |  |
| 0660 | 702000 | CONSTRUCTION SIGNING | S.F. | 100 |  |  |
| 0670 | 702100 | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING | L.F. | 50 |  |  |
| 0680 | 702101 | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING | EACH | 6 |  |  |
| 0690 | 702610 | PORTABLE CHANGEABLE MESSAGE SIGN | EACH | 4 |  |  |
| 0700 | 702612 | PORTABLE FLOODLIGHT SYSTEM | EACH | 2 |  |  |
| 0710 | 702710 | MOBILE TRAFFIC SIGNAL SYSTEM | EACH | 1 |  |  |
| 0720 | 702810 | TRAFFIC CONTROL DEVICES FOR CONSTRUCTION | LS | 1 |  |  |
| 0730 | 703100 | ROAD DELINEATOR TYPE GUIDE | EACH | 46 |  |  |
| 0740 | 704000 | RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 154400 |  |  |
| 0750 | 704005 | RETROREFLECTORIZED PAINTED MARKINGS 24" | L.F. | 50 |  |  |
| 0760 | 704009 | RETROREFLECTORIZED PAINTED MARKING RIGHT ARROW | EACH | 6 |  |  |
| 0770 | 704010 | RETROREFLECTORIZED PAINTED MARKING LEFT ARROW | EACH | 4 |  |  |
| 0780 | 704012 | RETROREFLECTORIZED PAINTED MARKING WORD (ONLY) | EACH | 3 |  |  |
| 0790 | 704027 | RETROREFLECTORIZED PAINTED MARKING RIGHT LANE DROP ARROW | EACH | 2 |  |  |
| 0800 | 704028 | RETROREFLECTORIZED PAINTED MARKING LEFT LANE DROP ARROW | EACH | 2 |  |  |
| 0810 | 704099 | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 25100 |  |  |
| 0820 | 704876 | TEMPORARY REFLECTIVE RAISED PAVEMENT MARKER, TYPE TG | EACH | 500 |  |  |
| 0830 | 704877 | TEMPORARY REFLECTIVE RAISED PAVEMENT MARKER, TYPE TH | EACH | 140 |  |  |
| 0840 | 706100 | SERVICE RISER (SIGNAL) | EACH | 1 |  |  |
| 0850 | 706200 | METER PEDESTAL (SIGNAL) | EACH | 1 |  |  |
| 0860 | 706350 | POWER SERVICE INSTALLATION | LS | 1 | $8,000.00 |  |
| 0870 | 711108 | SINGLE CONDUCTOR 8 | L.F. | 3690 |  |  |
| 0880 | 720050 | PERMANENT VEHICULAR IMPACT ATTENUATOR UNIT | EACH | 6 |  |  |
| 0890 | 720060 | VEHICULAR IMPACT ATTENUATOR UNIT-WORK ZONES | EACH | 18 |  |  |
| 0900 | 720110 | REMOVE/RESET IMPACT ATTENUATOR UNIT | EACH | 12 |  |  |
| 0910 | 750000 | INTELLIGENT TRANSPORTATION SYSTEM | LS | 1 |  |  |
| 0920 | 750022 | COMMUNICATIONS CONDUIT 2" | L.F. | 1310 |  |  |
| 0930 | 750023 | COMMUNICATIONS CONDUIT 3" | L.F. | 1310 |  |  |
| 0940 | 750060 | ITS PULLBOX (33"X24"X24") | EACH | 7 |  |  |
| 0950 | 750080 | ITS MANHOLE (48"X48"X48") | EACH | 1 |  |  |
| 0960 | 750100 | CLOSED CIRCUIT TELEVISION SYSTEM (CCTV) | EACH | 1 |  |  |
| 0970 | 750110 | CAMERA LOWERING DEVICE | EACH | 1 |  |  |
| 0980 | 750250 | ITS CONCRETE POLE, 50 FT | EACH | 1 |  |  |
| 0990 | 801000 | CONSTRUCTION STAKING BY THE CONTRACTOR | LS | 1 |  |  |
| 1000 | 802000 | POST CONSTRUCTION PLANS | LS | 1 | $15,000.00 |  |
| 1010 | 803000 | SCHEDULE SOFTWARE | LS | 1 |  |  |
| 1020 | 803020 | CPM HARDWARE/EQUIPMENT | LS | 1 |  |  |