Date Generated

**Apr 18, 2023**

Call Order

**001**

Project ID

**51011715101172R**

Amendments

**0**

Counties

**San Juan**

Highway Number

Time Remaining

Add to calendar

Days

**27**

Hours

**23**

Description

**Roadway Recon/Rehab, Bridge Replacement, ITS, Lighting**

Items



Edit favorites

Export

| **Line** | **Item** | **Description** | **Unit** | **Quantity** | **Price** |
| --- | --- | --- | --- | --- | --- |
| Section 0001: ROADWAY |
| 0010 | 201000 | CLEARING AND GRUBBING | LS | 1 |  |  |
| 0020 | 203000 | UNCLASSIFIED EXCAVATION | C.Y. | 54200 |  |  |
| 0030 | 203100 | BORROW | C.Y. | 116200 |  |  |
| 0040 | 203200 | UNSUITABLE MATERIAL EXCAVATION | C.Y. | 9100 |  |  |
| 0050 | 203211 | UNSTABLE SUBGRADE STABILIZATION | S.Y. | 33200 |  |  |
| 0060 | 203301 | ROCK EXCAVATION | C.Y. | 9690 |  |  |
| 0070 | 207000 | SUBGRADE PREPARATION | S.Y. | 204700 |  |  |
| 0080 | 302000 | PROCESSING, PLACING AND COMPACTING EXISTING PAVEMENT | S.Y. | 44000 |  |  |
| 0090 | 303000 | BASE COURSE | TON | 62600 |  |  |
| 0100 | 303140 | BASE COURSE 4" | S.Y. | 4000 |  |  |
| 0110 | 303160 | BASE COURSE 6" | S.Y. | 6900 |  |  |
| 0120 | 403701 | OPEN GRADED FRICTION COURSE COMPLETE | TON | 4340 |  |  |
| 0130 | 405000 | DETOUR PAVEMENT CONSTRUCTION | S.Y. | 32320 |  |  |
| 0140 | 407000 | ASPHALT MATERIAL FOR TACK COAT | TON | 123 |  |  |
| 0150 | 408100 | PRIME COAT MATERIAL | TON | 454 |  |  |
| 0160 | 416207 | MINOR PAVING TYPE II, HMA SP-IV | S.Y. | 9100 |  |  |
| 0170 | 417000 | MISCELLANEOUS PAVING | S.Y. | 3060 |  |  |
| 0180 | 423283 | HMA SP-IV COMPLETE | TON | 70700 |  |  |
| 0190 | 502030 | DRILLED SHAFT FOUNDATION 30" DIAMETER | L.F. | 100 |  |  |
| 0200 | 511000 | STRUCTURAL CONCRETE, CLASS A | C.Y. | 184 |  |  |
| 0210 | 511030 | STRUCTURAL CONCRETE, CLASS AA | C.Y. | 110 |  |  |
| 0220 | 511200 | STRUCTURAL CONCRETE, CLASS A-4" | S.Y. | 390 |  |  |
| 0230 | 515000 | REINF.CONCRETE FOR MINOR STRUCTURES | C.Y. | 82 |  |  |
| 0240 | 516000 | FLOWABLE FILL | C.Y. | 200 |  |  |
| 0250 | 519000 | STRUCTURAL SHOTCRETE | S.Y. | 160 |  |  |
| 0260 | 540060 | REINFORCING BARS GRADE 60 | LB | 23478 |  |  |
| 0270 | 541200 | STRUCTURAL STEEL FOR MISCELLANEOUS STRUCTURES | LB | 38200 |  |  |
| 0280 | 547000 | SAFETY AND ENVIRONMENTAL REQUIREMENTS | LS | 1 |  |  |
| 0290 | 570018 | 18" CULVERT PIPE | L.F. | 40 |  |  |
| 0300 | 570024 | 24" CULVERT PIPE | L.F. | 2530 |  |  |
| 0310 | 570025 | 24" CULVERT PIPE END SECTION | EACH | 16 |  |  |
| 0320 | 570030 | 30" CULVERT PIPE | L.F. | 820 |  |  |
| 0330 | 570031 | 30" CULVERT PIPE END SECTION | EACH | 8 |  |  |
| 0340 | 570036 | 36" CULVERT PIPE | L.F. | 830 |  |  |
| 0350 | 570037 | 36" CULVERT PIPE END SECTION | EACH | 12 |  |  |
| 0360 | 570042 | 42" CULVERT PIPE | L.F. | 170 |  |  |
| 0370 | 570043 | 42" CULVERT PIPE END SECTION | EACH | 2 |  |  |
| 0380 | 570060 | 60" CULVERT PIPE | L.F. | 190 |  |  |
| 0390 | 570061 | 60" CULVERT PIPE END SECTION | EACH | 2 |  |  |
| 0400 | 570096 | 96" CULVERT PIPE | L.F. | 140 |  |  |
| 0410 | 570950 | REINSTALLING CULVERT PIPE | L.F. | 140 |  |  |
| 0420 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| 0430 | 601110 | REMOVAL OF SURFACING | S.Y. | 139000 |  |  |
| 0440 | 602000 | RIPRAP CLASS A | C.Y. | 1250 |  |  |
| 0450 | 602010 | RIPRAP CLASS B | C.Y. | 80 |  |  |
| 0460 | 602020 | RIPRAP CLASS C | C.Y. | 60 |  |  |
| 0470 | 602060 | RIPRAP CLASS G | S.Y. | 10110 |  |  |
| 0480 | 602200 | GABIONS | C.Y. | 10 |  |  |
| 0490 | 603100 | TEMPORARY SOIL STABILANT | ACRE | 56 |  |  |
| 0500 | 603262 | COMPOSTED MULCH SOCKS | L.F. | 10600 |  |  |
| 0510 | 603281 | SWPPP PLAN PREPARATION AND MAINTENANCE | LS | 1 |  |  |
| 0520 | 606001 | SINGLE FACE W-BEAM GUARDRAIL | L.F. | 12500 |  |  |
| 0530 | 606051 | END TREATMENT TL-3 END TERMINAL | EACH | 35 |  |  |
| 0540 | 606055 | END TREATMENT DRIVEWAY END ANCHOR | EACH | 7 |  |  |
| 0550 | 606062 | TRANSITION METAL BARRIER TO RIGID BARRIER | EACH | 4 |  |  |
| 0560 | 606542 | CONCRETE WALL BARRIER 42" | L.F. | 590 |  |  |
| 0570 | 606710 | TCWB RETAINED BY THE CONTRACTOR (20') | L.F. | 5860 |  |  |
| 0580 | 606719 | RESETTING OF TCWB (20') | L.F. | 10660 |  |  |
| 0590 | 607014 | WOVEN WIRE FENCE 4' | L.F. | 86700 |  |  |
| 0600 | 607015 | BRACES/CORNER POSTS | EACH | 388 |  |  |
| 0610 | 607316 | STANDARD GATE, 16' | EACH | 9 |  |  |
| 0620 | 607326 | STANDARD GATE, 26' | EACH | 3 |  |  |
| 0630 | 608004 | CONCRETE SIDEWALK 4" | S.Y. | 110 |  |  |
| 0640 | 608304 | CONCRETE MEDIAN PAVEMENT 4" (COLORED) | S.Y. | 260 |  |  |
| 0650 | 609324 | CONCRETE SLOPED CURB AND GUTTER 6" X 24" | L.F. | 660 |  |  |
| 0660 | 609424 | CONCRETE VERTICAL CURB AND GUTTER TYPE B 6" X 24" | L.F. | 180 |  |  |
| 0670 | 610000 | CATTLE GUARD | L.F. | 546 |  |  |
| 0680 | 613000 | CLEANING CULVERTS AND DRAINAGE STRUCTURES | LS | 1 |  |  |
| 0690 | 618000 | TRAFFIC CONTROL MANAGEMENT | LS | 1 |  |  |
| 0700 | 618011 | PUBLIC AWARENESS | LS | 1 | $25,000.00 |  |
| 0710 | 621000 | MOBILIZATION | LS | 1 |  |  |
| 0720 | 622002 | FIELD LABORATORY, TYPE II | EACH | 1 |  |  |
| 0730 | 622100 | SUPPLEMENTAL FIELD LABORATORY | EACH | 1 |  |  |
| 0740 | 622110 | SUPPLEMENTAL HOT-MIX ASPHALT FIELD LABORATORY | EACH | 1 |  |  |
| 0750 | 622200 | FIELD OFFICE | EACH | 1 |  |  |
| 0760 | 631000 | RUMBLE STRIPS | L.F. | 91400 |  |  |
| 0770 | 632000 | CLASS A SEEDING | ACRE | 34 |  |  |
| 0780 | 632020 | CLASS C SEEDING | ACRE | 13 |  |  |
| 0790 | 663870 | BORING AND JACKING | L.F. | 1340 |  |  |
| 0800 | 667110 | MAIL BOX INSTALLATION-SINGLE | EACH | 2 |  |  |
| 0810 | 701000 | PANEL SIGNS | S.F. | 1920 |  |  |
| 0820 | 701030 | REMOVE AND RESET PANEL SIGN | EACH | 1 |  |  |
| 0830 | 701031 | REMOVE AND RESET TRAFFIC SIGN | EACH | 7 |  |  |
| 0840 | 701100 | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS | L.F. | 3540 |  |  |
| 0850 | 701109 | STEEL I-BEAM POST TYPE W6X9 | L.F. | 30 |  |  |
| 0860 | 701209 | BREAKAWAY BASE SYSTEM FOR STEEL I BEAM POST W6X9 | EACH | 2 |  |  |
| 0870 | 702000 | CONSTRUCTION SIGNING | S.F. | 200 |  |  |
| 0880 | 702100 | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING | L.F. | 180 |  |  |
| 0890 | 702101 | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING | EACH | 12 |  |  |
| 0900 | 702610 | PORTABLE CHANGEABLE MESSAGE SIGN | EACH | 4 |  |  |
| 0910 | 702612 | PORTABLE FLOODLIGHT SYSTEM | EACH | 5 |  |  |
| 0920 | 702710 | MOBILE TRAFFIC SIGNAL SYSTEM | EACH | 1 |  |  |
| 0930 | 702810 | TRAFFIC CONTROL DEVICES FOR CONSTRUCTION | LS | 1 |  |  |
| 0940 | 702811 | TRAFFIC CONTROL DEVICES FOR PEDESTRIAN AND BICYCLIST | LS | 1 |  |  |
| 0950 | 703002 | OBJECT MARKER TYPE 2 | EACH | 64 |  |  |
| 0960 | 703003 | OBJECT MARKER TYPE 3 | EACH | 12 |  |  |
| 0970 | 704000 | RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 548400 |  |  |
| 0980 | 704005 | RETROREFLECTORIZED PAINTED MARKINGS 24" | L.F. | 540 |  |  |
| 0990 | 704099 | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 771695 |  |  |
| 1000 | 704717 | HOT THERMOPLASTIC PAVEMENT MARKING RIGHT ARROW | EACH | 14 |  |  |
| 1010 | 704718 | HOT THERMOPLASTIC PAVEMENT MARKING LEFT ARROW | EACH | 20 |  |  |
| 1020 | 704720 | HOT THERMOPLASTIC PAVEMENT MARKING WORD (ONLY) | EACH | 17 |  |  |
| 1030 | 704735 | HOT THERMOPLASTIC PAVEMENT MARKING RIGHT LANE DROP ARROW | EACH | 3 |  |  |
| 1040 | 705000 | SIGNAL/LIGHTING SYSTEM START-UP COSTS | ALOW | 1 | $10,000.00 |  |
| 1050 | 706110 | SERVICE RISER (LIGHTING) | EACH | 1 |  |  |
| 1060 | 706350 | POWER SERVICE INSTALLATION | LS | 1 | $3,500.00 |  |
| 1070 | 706420 | LIGHTING CONTROL CABINET-TWO CIRCUIT | EACH | 1 |  |  |
| 1080 | 707540 | TYPE V STANDARD, 40' | EACH | 13 |  |  |
| 1090 | 707801 | REMOVE & RESET TYPE I STANDARD COMPLETE | EACH | 4 |  |  |
| 1100 | 709020 | RIGID ELECTRICAL CONDUIT 2" (DIA.) | L.F. | 7400 |  |  |
| 1110 | 709030 | RIGID ELECTRICAL CONDUIT 3" (DIA.) | L.F. | 630 |  |  |
| 1120 | 710000 | ELECTRICAL PULL BOX (STANDARD) | EACH | 34 |  |  |
| 1130 | 711102 | SINGLE CONDUCTOR 2 | L.F. | 15600 |  |  |
| 1140 | 711108 | SINGLE CONDUCTOR 8 | L.F. | 7800 |  |  |
| 1150 | 711230 | SINGLE CONDUCTOR 3/0 | L.F. | 120 |  |  |
| 1160 | 716701 | LED ROADWAY LUMINAIRE | EACH | 13 |  |  |
| 1170 | 720050 | PERMANENT VEHICULAR IMPACT ATTENUATOR UNIT | EACH | 4 |  |  |
| 1180 | 720060 | VEHICULAR IMPACT ATTENUATOR UNIT-WORK ZONES | EACH | 14 |  |  |
| 1190 | 720100 | SAND BARREL VEHICULAR IMPACT ATTENUATOR UNIT | EACH | 1 |  |  |
| 1200 | 720110 | REMOVE/RESET IMPACT ATTENUATOR UNIT | EACH | 46 |  |  |
| 1210 | 721000 | REMOVAL OF PAVEMENT MARKING | L.F. | 268276 |  |  |
| 1220 | 721101 | REMOVAL OF PAVEMENT MARKING SYMBOL | EACH | 10 |  |  |
| 1230 | 750000 | INTELLIGENT TRANSPORTATION SYSTEM | LS | 1 |  |  |
| 1240 | 750032 | MULTI-DUCT CONDUIT 2" (8-WAY) | L.F. | 86100 |  |  |
| 1250 | 750060 | ITS PULLBOX (33"X24"X24") | EACH | 37 |  |  |
| 1260 | 750080 | ITS MANHOLE (48"X48"X48") | EACH | 7 |  |  |
| 1270 | 801000 | CONSTRUCTION STAKING BY THE CONTRACTOR | LS | 1 |  |  |
| 1280 | 802000 | POST CONSTRUCTION PLANS | LS | 1 | $95,000.00 |  |
| 1290 | 803000 | SCHEDULE SOFTWARE | LS | 1 |  |  |
| Section 0002: BRIDGE |
| 1300 | 203100 | BORROW | C.Y. | 10 |  |  |
| 1310 | 203301 | ROCK EXCAVATION | C.Y. | 1519 |  |  |
| 1320 | 207000 | SUBGRADE PREPARATION | S.Y. | 130 |  |  |
| 1330 | 210001 | UNSUITABLE MATERIAL EXCAVATION | C.Y. | 460 |  |  |
| 1340 | 210002 | MAJOR STRUCTURE EXCAVATION | C.Y. | 3358 |  |  |
| 1350 | 210003 | MAJOR STRUCTURE BACKFILL | C.Y. | 6278 |  |  |
| 1360 | 411000 | HOT POURED CRACK SEALING | LB | 24 |  |  |
| 1370 | 502036 | DRILLED SHAFT FOUNDATION 36" DIAMETER | L.F. | 464 |  |  |
| 1380 | 502048 | DRILLED SHAFT FOUNDATION 48" DIAMETER | L.F. | 336 |  |  |
| 1390 | 502154 | PERMANENT CASING 54" DIAMETER | L.F. | 288 |  |  |
| 1400 | 502600 | OBSTRUCTION REMOVAL | L.F. | 81 |  |  |
| 1410 | 505000 | CROSSHOLE SONIC LOGGING CONSULTANT TESTING | EACH | 16 |  |  |
| 1420 | 505011 | LOW STRAIN INTEGRITY CONSULTANT TESTING | EACH | 16 |  |  |
| 1430 | 506000 | MSE PANEL WALL | S.F. | 6260 |  |  |
| 1440 | 511000 | STRUCTURAL CONCRETE, CLASS A | C.Y. | 330 |  |  |
| 1450 | 511030 | STRUCTURAL CONCRETE, CLASS AA | C.Y. | 840 |  |  |
| 1460 | 511070 | STRUCTURAL CONCRETE, CLASS HPD | C.Y. | 612 |  |  |
| 1470 | 518054 | PRESTRESSED CONCRETE BRIDGE MEMBER TYPE 54 | L.F. | 1296 |  |  |
| 1480 | 519001 | NON STRUCTURAL SHOTCRETE | S.Y. | 230 |  |  |
| 1490 | 536001 | EPOXY URETHANE POLYMER CONCRETE BRIDGE DECK OVERLAY | S.Y. | 1496 |  |  |
| 1500 | 540060 | REINFORCING BARS GRADE 60 | LB | 301461 |  |  |
| 1510 | 540061 | GALVANIZED BARS GRADE 60 | LB | 123963 |  |  |
| 1520 | 541000 | STRUCTURAL STEEL FOR CONCRETE BRIDGES | LB | 14669 |  |  |
| 1530 | 541200 | STRUCTURAL STEEL FOR MISCELLANEOUS STRUCTURES | LB | 360 |  |  |
| 1540 | 543002 | METAL RAILING, TYPE A42 | L.F. | 607 |  |  |
| 1550 | 560000 | ELASTOMERIC BEARING PADS | EACH | 30 |  |  |
| 1560 | 562000 | BRIDGE JOINT STRIP SEAL | L.F. | 104 |  |  |
| 1570 | 563099 | POLYMER BRIDGE JOINT SEALS | L.F. | 100 |  |  |
| 1580 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| 1590 | 602003 | RIPRAP CLASS A (MODIFIED) | C.Y. | 400 |  |  |
| 1600 | 602200 | GABIONS | C.Y. | 430 |  |  |
| 1610 | 604300 | GEOGRID REINFORCEMENT | S.Y. | 4366 |  |  |

Date Generated

**Apr 18, 2023**

Call Order

**002**

Project ID

**4100384R**

Amendments

**0**

Counties

**Colfax Mora**

Highway Number

Time Remaining

Add to calendar

Days

**27**

Hours

**23**

Description

**Roadway Reconstruction**

Items

Favorite items only

Edit favorites

Export

| **Line** | **Item** | **Description** | **Unit** | **Quantity** | **Price** |
| --- | --- | --- | --- | --- | --- |
| Section 0001: ROADWAY |
| 0010 | 201000 | CLEARING AND GRUBBING | LS | 1 |  |  |
| 0020 | 203000 | UNCLASSIFIED EXCAVATION | C.Y. | 22300 |  |  |
| 0030 | 203100 | BORROW | C.Y. | 3800 |  |  |
| 0040 | 203211 | UNSTABLE SUBGRADE STABILIZATION | S.Y. | 8460 |  |  |
| 0050 | 203300 | CONTROLLED BLASTING | L.F. | 12500 |  |  |
| 0060 | 203301 | ROCK EXCAVATION | C.Y. | 7900 |  |  |
| 0070 | 206000 | UNSUITABLE MATERIAL EXCAVATION | C.Y. | 10 |  |  |
| 0080 | 207000 | SUBGRADE PREPARATION | S.Y. | 35260 |  |  |
| 0090 | 303000 | BASE COURSE | TON | 10807 |  |  |
| 0100 | 405000 | DETOUR PAVEMENT CONSTRUCTION | S.Y. | 15700 |  |  |
| 0110 | 407000 | ASPHALT MATERIAL FOR TACK COAT | TON | 14 |  |  |
| 0120 | 408100 | PRIME COAT MATERIAL | TON | 69 |  |  |
| 0130 | 416213 | MINOR PAVING TYPE II, WMA SP-III | TON | 1430 |  |  |
| 0140 | 424003 | WMA SP-III COMPLETE | TON | 10120 |  |  |
| 0150 | 570024 | 24" CULVERT PIPE | L.F. | 648 |  |  |
| 0160 | 570025 | 24" CULVERT PIPE END SECTION | EACH | 25 |  |  |
| 0170 | 570162 | 42"SX29"R (NOMINAL) CULVERT PIPE ARCH | L.F. | 184 |  |  |
| 0180 | 570163 | 42"SX29"R (NOMINAL) CULVERT PIPE ARCH END SECTION | EACH | 6 |  |  |
| 0190 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| 0200 | 601110 | REMOVAL OF SURFACING | S.Y. | 23260 |  |  |
| 0210 | 602000 | RIPRAP CLASS A | C.Y. | 74 |  |  |
| 0220 | 602005 | RIPRAP CLASS A (NON-ENCLOSED) | C.Y. | 1190 |  |  |
| 0230 | 602110 | CONCRETE BLOCK REVETMENT | S.Y. | 800 |  |  |
| 0240 | 602200 | GABIONS | C.Y. | 100 |  |  |
| 0250 | 603100 | TEMPORARY SOIL STABILANT | ACRE | 12 |  |  |
| 0260 | 603221 | ROCK CHECK DAM | L.F. | 410 |  |  |
| 0270 | 603262 | COMPOSTED MULCH SOCKS | L.F. | 1370 |  |  |
| 0280 | 603281 | SWPPP PLAN PREPARATION AND MAINTENANCE | LS | 1 |  |  |
| 0290 | 604002 | GEOTEXTILE CLASS 2 | S.Y. | 42290 |  |  |
| 0300 | 604310 | GEOGRID BASE REINFORCEMENT | S.Y. | 42290 |  |  |
| 0310 | 606598 | TCWB RETAINED BY THE CONTRACTOR | L.F. | 1600 |  |  |
| 0320 | 606599 | RESETTING OF TCWB | L.F. | 1600 |  |  |
| 0330 | 607010 | BARBED WIRE FENCE (GAME FENCE) 4' | L.F. | 23280 |  |  |
| 0340 | 607015 | BRACES/CORNER POSTS | EACH | 102 |  |  |
| 0350 | 607316 | STANDARD GATE, 16' | EACH | 13 |  |  |
| 0360 | 607318 | STANDARD GATE, 18' | EACH | 1 |  |  |
| 0370 | 607326 | STANDARD GATE, 26' | EACH | 2 |  |  |
| 0380 | 610000 | CATTLE GUARD | L.F. | 30 |  |  |
| 0390 | 618000 | TRAFFIC CONTROL MANAGEMENT | LS | 1 |  |  |
| 0400 | 618011 | PUBLIC AWARENESS | LS | 1 |  |  |
| 0410 | 621000 | MOBILIZATION | LS | 1 |  |  |
| 0420 | 622002 | FIELD LABORATORY, TYPE II | EACH | 1 |  |  |
| 0430 | 622100 | SUPPLEMENTAL FIELD LABORATORY | EACH | 1 |  |  |
| 0440 | 622110 | SUPPLEMENTAL HOT-MIX ASPHALT FIELD LABORATORY | EACH | 1 |  |  |
| 0450 | 623011 | MEDIAN DROP INLET TYPE I (RURAL) H=0'0" TO 3'0" | EACH | 5 |  |  |
| 0460 | 624100 | SLOPE PROTECTION WIRE MESH PVC COATED | S.Y. | 2500 |  |  |
| 0470 | 624200 | RESIN GROUTED STEEL BOLTS | L.F. | 300 |  |  |
| 0480 | 624300 | RESIN GROUTED STEEL ANCHORS | L.F. | 1260 |  |  |
| 0490 | 626001 | LIGHT SCALING OF ROCK SLOPES | S.Y. | 1800 |  |  |
| 0500 | 626002 | HEAVY SCALING OF ROCK SLOPES | S.Y. | 300 |  |  |
| 0510 | 632000 | CLASS A SEEDING | ACRE | 5 |  |  |
| 0520 | 632005 | MODIFIED CLASS A SEEDING | ACRE | 1 |  |  |
| 0530 | 632020 | CLASS C SEEDING | ACRE | 4 |  |  |
| 0540 | 680002 | ROCK ANCHOR INSTALLATION | LS | 1 |  |  |
| 0550 | 701000 | PANEL SIGNS | S.F. | 150 |  |  |
| 0560 | 701030 | REMOVE AND RESET PANEL SIGN | EACH | 1 |  |  |
| 0570 | 701100 | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS | L.F. | 660 |  |  |
| 0580 | 702000 | CONSTRUCTION SIGNING | S.F. | 60 |  |  |
| 0590 | 702100 | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING | L.F. | 60 |  |  |
| 0600 | 702610 | PORTABLE CHANGEABLE MESSAGE SIGN | EACH | 3 |  |  |
| 0610 | 702612 | PORTABLE FLOODLIGHT SYSTEM | EACH | 4 |  |  |
| 0620 | 702710 | MOBILE TRAFFIC SIGNAL SYSTEM | EACH | 2 |  |  |
| 0630 | 702810 | TRAFFIC CONTROL DEVICES FOR CONSTRUCTION | LS | 1 |  |  |
| 0640 | 702850 | LAW ENFORCEMENT IN CONSTRUCTION ZONE | ALOW | 1 | $15,000.00 |  |
| 0650 | 703002 | OBJECT MARKER TYPE 2 | EACH | 36 |  |  |
| 0660 | 704000 | RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 94320 |  |  |
| 0670 | 704099 | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 1200 |  |  |
| 0680 | 720060 | VEHICULAR IMPACT ATTENUATOR UNIT-WORK ZONES | EACH | 4 |  |  |
| 0690 | 720110 | REMOVE/RESET IMPACT ATTENUATOR UNIT | EACH | 4 |  |  |
| 0700 | 801000 | CONSTRUCTION STAKING BY THE CONTRACTOR | LS | 1 |  |  |
| 0710 | 802000 | POST CONSTRUCTION PLANS | LS | 1 | $15,000.00 |  |
| 0720 | 803000 | SCHEDULE SOFTWARE | LS | 1 |  |  |
| 0730 | 803020 | CPM HARDWARE/EQUIPMENT | LS | 1 |  |  |

Date Generated

**Apr 18, 2023**

Call Order

**003**

Project ID

**1101022**

Amendments

**0**

Counties

**Dona Ana**

Highway Number

Time Remaining

Add to calendar

Days

**27**

Hours

**23**

Description

**Bridge Rehabilitation**

Items

Favorite items only

Edit favorites

Export

| **Line** | **Item** | **Description** | **Unit** | **Quantity** | **Price** |
| --- | --- | --- | --- | --- | --- |
| Section 0001: BRIDGE |
| 0010 | 452100 | RESEALING CONCRETE PAVEMENT JOINTS | L.F. | 68 |  |  |
| 0020 | 529000 | PIER AND ABUTMENT BEARING MODIFICATIONS | LS | 1 |  |  |
| 0030 | 533000 | REPAIR OF CONCRETE STRUCTURES | S.Y. | 155 |  |  |
| 0040 | 533001 | EMBEDDED GALVANIC ANODES | EACH | 360 |  |  |
| 0050 | 533003 | REPLACEMENT REINFORCING BARS | LB | 470 |  |  |
| 0060 | 534000 | EPOXY INJECTION, TYPE I | GAL | 10 |  |  |
| 0070 | 536001 | EPOXY URETHANE POLYMER CONCRETE BRIDGE DECK OVERLAY | S.Y. | 714 |  |  |
| 0080 | 541000 | STRUCTURAL STEEL FOR CONCRETE BRIDGES | LB | 11040 |  |  |
| 0090 | 546000 | RECOATING STRUCTURES | LS | 1 |  |  |
| 0100 | 546200 | SP 3 POWER TOOL CLEANING | S.F. | 200 |  |  |
| 0110 | 548002 | COATING OF CONCRETE - PAINT | S.F. | 5390 |  |  |
| 0120 | 560000 | ELASTOMERIC BEARING PADS | EACH | 46 |  |  |
| 0130 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| Section 0002: ROADWAY |
| 0140 | 547000 | SAFETY AND ENVIRONMENTAL REQUIREMENTS | LS | 1 |  |  |
| 0150 | 618000 | TRAFFIC CONTROL MANAGEMENT | LS | 1 |  |  |
| 0160 | 621000 | MOBILIZATION | LS | 1 |  |  |
| 0170 | 702000 | CONSTRUCTION SIGNING | S.F. | 1340 |  |  |
| 0180 | 702100 | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING | L.F. | 3420 |  |  |
| 0190 | 702101 | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING | EACH | 6 |  |  |
| 0200 | 702110 | PORTABLE SIGN SUPPORT | EACH | 24 |  |  |
| 0210 | 702238 | BARRICADE, TYPE III-8' | EACH | 7 |  |  |
| 0220 | 702320 | VERTICAL PANEL, TYPE BACK TO BACK | EACH | 20 |  |  |
| 0230 | 702525 | CHANNELIZATION DEVICES TYPE DRUM | EACH | 54 |  |  |
| 0240 | 702600 | SEQUENTIAL ARROW DISPLAY | EACH | 2 |  |  |
| 0250 | 702610 | PORTABLE CHANGEABLE MESSAGE SIGN | EACH | 7 |  |  |
| 0260 | 704100 | REMOVABLE MARKING TAPE 4" | L.F. | 500 |  |  |
| 0270 | 704700 | HOT THERMOPLASTIC PAVEMENT MARKINGS 4" | L.F. | 1000 |  |  |
| 0280 | 721000 | REMOVAL OF PAVEMENT MARKING | L.F. | 700 |  |  |
| 0290 | 801000 | CONSTRUCTION STAKING BY THE CONTRACTOR | LS | 1 |  |  |
| 0300 | 802000 | POST CONSTRUCTION PLANS | LS | 1 | $5,000.00 |  |

Date Generated

**Apr 18, 2023**

Call Order

**004**

Project ID

**5101710**

Amendments

**0**

Counties

**Santa Fe**

Highway Number

Time Remaining

Add to calendar

Days

**27**

Hours

**23**

Description

**Bridge Rehabilitation**

Items

Favorite items only

Edit favorites

Export

| **Line** | **Item** | **Description** | **Unit** | **Quantity** | **Price** |
| --- | --- | --- | --- | --- | --- |
| Section 0001: BRIDGE |
| 0010 | 203100 | BORROW | C.Y. | 60 |  |  |
| 0020 | 210003 | MAJOR STRUCTURE BACKFILL | C.Y. | 64 |  |  |
| 0030 | 411000 | HOT POURED CRACK SEALING | LB | 444 |  |  |
| 0040 | 452000 | SEALING CONCRETE PAVEMENT JOINTS | L.F. | 974 |  |  |
| 0050 | 511070 | STRUCTURAL CONCRETE, CLASS HPD | C.Y. | 25 |  |  |
| 0060 | 511200 | STRUCTURAL CONCRETE, CLASS A-4" | S.Y. | 180 |  |  |
| 0070 | 515000 | REINF.CONCRETE FOR MINOR STRUCTURES | C.Y. | 12 |  |  |
| 0080 | 516000 | FLOWABLE FILL | C.Y. | 20 |  |  |
| 0090 | 533000 | REPAIR OF CONCRETE STRUCTURES | S.Y. | 62 |  |  |
| 0100 | 533001 | EMBEDDED GALVANIC ANODES | EACH | 114 |  |  |
| 0110 | 533003 | REPLACEMENT REINFORCING BARS | LB | 50 |  |  |
| 0120 | 534000 | EPOXY INJECTION, TYPE I | GAL | 2 |  |  |
| 0130 | 534010 | EPOXY INJECTION, TYPE II | GAL | 2 |  |  |
| 0140 | 535100 | CONCRETE SURFACE TREATMENT | S.Y. | 5786 |  |  |
| 0150 | 536001 | EPOXY URETHANE POLYMER CONCRETE BRIDGE DECK OVERLAY | S.Y. | 7393 |  |  |
| 0160 | 540076 | UNCOATED CORROSION RESISTANT REINFORCING BARS GRADE 75 | LB | 3000 |  |  |
| 0170 | 541200 | STRUCTURAL STEEL FOR MISCELLANEOUS STRUCTURES | LB | 100 |  |  |
| 0180 | 562000 | BRIDGE JOINT STRIP SEAL | L.F. | 217 |  |  |
| 0190 | 563099 | POLYMER BRIDGE JOINT SEALS | L.F. | 585 |  |  |
| 0200 | 565000 | PREFORMED SILICONE-COATED FOAM JOINT SYSTEM | L.F. | 22 |  |  |
| 0210 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| 0220 | 602060 | RIPRAP CLASS G | S.Y. | 27 |  |  |
| 0230 | 602200 | GABIONS | C.Y. | 28 |  |  |
| Section 0002: ROADWAY |
| 0240 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| 0250 | 606001 | SINGLE FACE W-BEAM GUARDRAIL | L.F. | 250 |  |  |
| 0260 | 606051 | END TREATMENT TL-3 END TERMINAL | EACH | 2 |  |  |
| 0270 | 606062 | TRANSITION METAL BARRIER TO RIGID BARRIER | EACH | 2 |  |  |
| 0280 | 618000 | TRAFFIC CONTROL MANAGEMENT | LS | 1 |  |  |
| 0290 | 618011 | PUBLIC AWARENESS | LS | 1 | $21,000.00 |  |
| 0300 | 621000 | MOBILIZATION | LS | 1 |  |  |
| 0310 | 702000 | CONSTRUCTION SIGNING | S.F. | 91 |  |  |
| 0320 | 702100 | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING | L.F. | 98 |  |  |
| 0330 | 702101 | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING | EACH | 30 |  |  |
| 0340 | 702810 | TRAFFIC CONTROL DEVICES FOR CONSTRUCTION | LS | 1 |  |  |
| 0350 | 704000 | RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 9342 |  |  |
| 0360 | 704002 | RETROREFLECTORIZED PAINTED MARKINGS 6" | L.F. | 459 |  |  |
| 0370 | 704099 | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 200 |  |  |
| 0380 | 721000 | REMOVAL OF PAVEMENT MARKING | L.F. | 200 |  |  |
| 0390 | 802000 | POST CONSTRUCTION PLANS | LS | 1 | $28,500.00 |  |
| 0400 | 803000 | SCHEDULE SOFTWARE | LS | 1 |  |  |

Date Generated

**Apr 18, 2023**

Call Order

**005**

Project ID

**5101700**

Amendments

**0**

Counties

**Rio Arriba Santa Fe**

Highway Number

Time Remaining

Add to calendar

Days

**27**

Hours

**22**

Description

**Bridge Rehabilitation**

Items

Favorite items only

Edit favorites

Export

| **Line** | **Item** | **Description** | **Unit** | **Quantity** | **Price** |
| --- | --- | --- | --- | --- | --- |
| Section 0001: BRIDGE |
| 0010 | 203000 | UNCLASSIFIED EXCAVATION | C.Y. | 200 |  |  |
| 0020 | 210002 | MAJOR STRUCTURE EXCAVATION | C.Y. | 340 |  |  |
| 0030 | 210003 | MAJOR STRUCTURE BACKFILL | C.Y. | 210 |  |  |
| 0040 | 411000 | HOT POURED CRACK SEALING | LB | 108 |  |  |
| 0050 | 417000 | MISCELLANEOUS PAVING | S.Y. | 7 |  |  |
| 0060 | 511000 | STRUCTURAL CONCRETE, CLASS A | C.Y. | 200 |  |  |
| 0070 | 511070 | STRUCTURAL CONCRETE, CLASS HPD | C.Y. | 3 |  |  |
| 0080 | 516000 | FLOWABLE FILL | C.Y. | 10 |  |  |
| 0090 | 533003 | REPLACEMENT REINFORCING BARS | LB | 105 |  |  |
| 0100 | 540060 | REINFORCING BARS GRADE 60 | LB | 16000 |  |  |
| 0110 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| 0120 | 602000 | RIPRAP CLASS A | C.Y. | 70 |  |  |
| 0130 | 602200 | GABIONS | C.Y. | 20 |  |  |
| 0140 | 623345 | CURB DROP INLET FOR CONCRETE WALL BARRIER | EACH | 1 |  |  |
| Section 0002: ROADWAY |
| 0150 | 603100 | TEMPORARY SOIL STABILANT | ACRE | 1 |  |  |
| 0160 | 606001 | SINGLE FACE W-BEAM GUARDRAIL | L.F. | 287.5 |  |  |
| 0170 | 606051 | END TREATMENT TL-3 END TERMINAL | EACH | 2 |  |  |
| 0180 | 606053 | END TREATMENT W-BEAM END ANCHOR | EACH | 1 |  |  |
| 0190 | 606062 | TRANSITION METAL BARRIER TO RIGID BARRIER | EACH | 1 |  |  |
| 0200 | 606542 | CONCRETE WALL BARRIER 42" | L.F. | 118 |  |  |
| 0210 | 613000 | CLEANING CULVERTS AND DRAINAGE STRUCTURES | LS | 1 |  |  |
| 0220 | 618000 | TRAFFIC CONTROL MANAGEMENT | LS | 1 |  |  |
| 0230 | 618011 | PUBLIC AWARENESS | LS | 1 | $14,000.00 |  |
| 0240 | 621000 | MOBILIZATION | LS | 1 |  |  |
| 0250 | 632020 | CLASS C SEEDING | ACRE | 1 |  |  |
| 0260 | 701030 | REMOVE AND RESET PANEL SIGN | EACH | 2 |  |  |
| 0270 | 702000 | CONSTRUCTION SIGNING | S.F. | 50 |  |  |
| 0280 | 702100 | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING | L.F. | 50 |  |  |
| 0290 | 702810 | TRAFFIC CONTROL DEVICES FOR CONSTRUCTION | LS | 1 |  |  |
| 0300 | 704000 | RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 700 |  |  |
| 0310 | 704099 | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 270 |  |  |
| 0320 | 721000 | REMOVAL OF PAVEMENT MARKING | L.F. | 600 |  |  |
| 0330 | 801000 | CONSTRUCTION STAKING BY THE CONTRACTOR | LS | 1 |  |  |
| 0340 | 802000 | POST CONSTRUCTION PLANS | LS | 1 | $18,000.00 |  |
| 0350 | 803000 | SCHEDULE SOFTWARE | LS | 1 |  |  |