|  |  |  |
| --- | --- | --- |
|  | **Proposal 1101021** |  |

Roadway Reconstruction/Rehabilitation, Weigh-in-Motion

|  |  |  |  |
| --- | --- | --- | --- |
| Proposal information table | | | |
| **Date Generated:** | 07/22/2020 | **Sections:** | 1 |
| **Date Revised:** |  | **Amendments:** | 0 |
| **Call Order:** | 001 | **Highway Number:** |  |
| **Items:** | 72 | **Counties:** | Dona Ana |
| **Project ID:** | 1101021 |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Proposal items table | | | | | |
| **Line** | **Item** | **Quantity** | **Unit** | **Description** | **Price** |
| **Section 0001: ROADWAY** | | | | | |
| 0010 | 201000 | 1.000 | LS | CLEARING AND GRUBBING |  |
| 0020 | 203000 | 238,300.000 | C.Y. | UNCLASSIFIED EXCAVATION |  |
| 0030 | 203100 | 1,300.000 | C.Y. | BORROW |  |
| 0040 | 207000 | 368,563.000 | S.Y. | SUBGRADE PREPARATION |  |
| 0050 | 209000 | 3.700 | MILE | BLADING AND RESHAPING |  |
| 0060 | 213000 | 0.280 | MILE | OBLITERATING OLD ROAD |  |
| 0070 | 303000 | 421,996.000 | TON | BASE COURSE |  |
| 0080 | 403715 | 2,881.000 | TON | RUBBERIZED OPEN-GRADED FRICTION COURSE COMPLETE |  |
| 0090 | 407000 | 172.000 | TON | ASPHALT MATERIAL FOR TACK COAT |  |
| 0100 | 408100 | 488.000 | TON | PRIME COAT MATERIAL |  |
| 0110 | 414000 | 34,904.000 | SYIN | COLD MILLING (ASPHALT) |  |
| 0120 | 423283 | 86,664.000 | TON | HMA SP-IV COMPLETE |  |
| 0130 | 515000 | 11.000 | C.Y. | REINF.CONCRETE FOR MINOR STRUCTURES |  |
| 0140 | 516000 | 52.000 | C.Y. | FLOWABLE FILL |  |
| 0150 | 541200 | 200.000 | LB | STRUCTURAL STEEL FOR MISCELLANEOUS STRUCTURES |  |
| 0160 | 601000 | 1.000 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  |
| 0170 | 601110 | 166,737.000 | S.Y. | REMOVAL OF SURFACING |  |
| 0180 | 602060 | 4,218.000 | S.Y. | RIPRAP CLASS G |  |
| 0190 | 603100 | 26.000 | ACRE | TEMPORARY SOIL STABILANT |  |
| 0200 | 603221 | 50.000 | L.F. | CHECK DAM TYPE II |  |
| 0210 | 603262 | 6,500.000 | L.F. | COMPOSTED MULCH SOCKS |  |
| 0220 | 603281 | 1.000 | LS | SWPPP PLAN PREPARATION AND MAINTENANCE |  |
| 0230 | 604003 | 342,045.000 | S.Y. | GEOTEXTILE CLASS 3 |  |
| 0240 | 604300 | 855,534.000 | S.Y. | GEOGRID REINFORCEMENT |  |
| 0250 | 606001 | 5,287.500 | L.F. | SINGLE FACE W-BEAM GUARDRAIL |  |
| 0260 | 606051 | 10.000 | EACH | END TREATMENT TL-3 END TERMINAL |  |
| 0270 | 606053 | 4.000 | EACH | END TREATMENT W-BEAM END ANCHOR |  |
| 0280 | 606062 | 10.000 | EACH | TRANSITION METAL BARRIER TO RIGID BARRIER |  |
| 0290 | 606542 | 170.000 | L.F. | CONCRETE WALL BARRIER 42" |  |
| 0300 | 606600 | 3,620.000 | L.F. | TCWB RETAINED BY THE DEPARTMENT (10') |  |
| 0310 | 606610 | 21,380.000 | L.F. | TCWB RETAINED BY THE CONTRACTOR (10') |  |
| 0320 | 606619 | 28,620.000 | L.F. | RESETTING OF TCWB (10') |  |
| 0330 | 609430 | 330.000 | L.F. | CONCRETE VERTICAL CURB AND GUTTER TYPE B 6" X 30" |  |
| 0340 | 609478 | 3,550.000 | L.F. | CONCRETE VERTICAL CURB AND GUTTER TYPE D 6" X 18" |  |
| 0350 | 613000 | 1.000 | LS | CLEANING CULVERTS AND DRAINAGE STRUCTURES |  |
| 0360 | 618000 | 1.000 | LS | TRAFFIC CONTROL MANAGEMENT |  |
| 0370 | 621000 | 1.000 | LS | MOBILIZATION |  |
| 0380 | 630100 | 3,000.000 | L.F. | MULTIPLE GLARE SHIELDING 24 IN |  |
| 0390 | 631000 | 74,166.000 | L.F. | RUMBLE STRIPS |  |
| 0400 | 632000 | 17.000 | ACRE | CLASS A SEEDING |  |
| 0410 | 632020 | 5.000 | ACRE | CLASS C SEEDING |  |
| 0420 | 701000 | 600.000 | S.F. | PANEL SIGNS |  |
| 0430 | 701100 | 1,135.000 | L.F. | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS |  |
| 0440 | 702000 | 1,115.000 | S.F. | CONSTRUCTION SIGNING |  |
| 0450 | 702100 | 3,867.000 | L.F. | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING |  |
| 0460 | 702101 | 12.000 | EACH | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING |  |
| 0470 | 702238 | 2.000 | EACH | BARRICADE, TYPE III-8' |  |
| 0480 | 702525 | 202.000 | EACH | CHANNELIZATION DEVICES TYPE DRUM |  |
| 0490 | 702600 | 2.000 | EACH | SEQUENTIAL ARROW DISPLAY |  |
| 0500 | 702610 | 4.000 | EACH | PORTABLE CHANGEABLE MESSAGE SIGN |  |
| 0510 | 703002 | 32.000 | EACH | OBJECT MARKER TYPE 2 |  |
| 0520 | 703100 | 352.000 | EACH | ROAD DELINEATOR TYPE GUIDE |  |
| 0530 | 703400 | 74.000 | EACH | 1/10TH MILE DELINEATOR |  |
| 0540 | 704099 | 204,600.000 | L.F. | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" |  |
| 0550 | 704700 | 12,180.000 | L.F. | HOT THERMOPLASTIC PAVEMENT MARKINGS 4" |  |
| 0560 | 704701 | 89,775.000 | L.F. | HOT THERMOPLASTIC PAVEMENT MARKINGS 6" |  |
| 0570 | 704704 | 37.000 | L.F. | HOT THERMOPLASTIC PAVEMENT MARKING 24" |  |
| 0580 | 704706 | 4,200.000 | L.F. | HOT THERMOPLASTIC PAVEMENT MARKINGS 12" |  |
| 0590 | 704728 | 16.000 | L.F. | HOT THERMOPLASTIC PAVEMENT MARKING YIELD LINE |  |
| 0600 | 704871 | 2,080.000 | EACH | PLOWABLE REFLECTIVE RAISED PAVEMENT MARKER TYPE PJ |  |
| 0610 | 704872 | 1,050.000 | EACH | PLOWABLE REFLECTIVE RAISED PAVEMENT MARKER TYPE PC |  |
| 0620 | 704876 | 1,691.000 | EACH | TEMPORARY REFLECTIVE RAISED PAVEMENT MARKER, TYPE TG |  |
| 0630 | 704877 | 1,716.000 | EACH | TEMPORARY REFLECTIVE RAISED PAVEMENT MARKER, TYPE TH |  |
| 0640 | 704939 | 6.000 | EACH | PREFORMED THERMOPLASTIC PAVEMENT MARKING WRONG WAY ARROW |  |
| 0650 | 720060 | 3.000 | EACH | VEHICULAR IMPACT ATTENUATOR UNIT-WORK ZONES |  |
| 0660 | 720110 | 3.000 | EACH | REMOVE/RESET IMPACT ATTENUATOR UNIT |  |
| 0670 | 721000 | 186,000.000 | L.F. | REMOVAL OF PAVEMENT MARKING |  |
| 0680 | 730200 | 1.000 | LS | WEIGH-IN-MOTION SYSTEM |  |
| 0690 | 801000 | 1.000 | LS | CONSTRUCTION STAKING BY THE CONTRACTOR |  |
| 0700 | 802000 | 1.000 | LS | POST CONSTRUCTION PLANS | $5,000.00000 |
| 0710 | 803000 | 1.000 | LS | SCHEDULE SOFTWARE |  |
| 0720 | 803020 | 1.000 | LS | CPM HARDWARE/EQUIPMENT |  |

|  |  |  |
| --- | --- | --- |
|  | **Proposal E100202** |  |

Roadway Recon, Bridge Rpl, Signal, Lighting, ITS

|  |  |  |  |
| --- | --- | --- | --- |
| Proposal information table | | | |
| **Date Generated:** | 07/22/2020 | **Sections:** | 2 |
| **Date Revised:** |  | **Amendments:** | 0 |
| **Call Order:** | 002 | **Highway Number:** |  |
| **Items:** | 179 | **Counties:** | Dona Ana |
| **Project ID:** | E100202 |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Proposal items table | | | | | |
| **Line** | **Item** | **Quantity** | **Unit** | **Description** | **Price** |
| **Section 0001: ROADWAY** | | | | | |
| 0010 | 201000 | 1.000 | LS | CLEARING AND GRUBBING |  |
| 0020 | 203000 | 28,200.000 | C.Y. | UNCLASSIFIED EXCAVATION |  |
| 0030 | 203100 | 21,400.000 | C.Y. | BORROW |  |
| 0040 | 203211 | 8,200.000 | S.Y. | UNSTABLE SUBGRADE STABILIZATION |  |
| 0050 | 207000 | 56,100.000 | S.Y. | SUBGRADE PREPARATION |  |
| 0060 | 303000 | 16,210.000 | TON | BASE COURSE |  |
| 0070 | 405000 | 16,900.000 | S.Y. | DETOUR PAVEMENT CONSTRUCTION |  |
| 0080 | 407000 | 16.000 | TON | ASPHALT MATERIAL FOR TACK COAT |  |
| 0090 | 408100 | 61.000 | TON | PRIME COAT MATERIAL |  |
| 0100 | 416014 | 9,630.000 | TON | MINOR PAVEMENT HMA SP-IV |  |
| 0110 | 417000 | 3,900.000 | S.Y. | MISCELLANEOUS PAVING |  |
| 0120 | 450090 | 19,940.000 | S.Y. | CONCRETE PAVEMENT-9" |  |
| 0130 | 455000 | 19,940.000 | S.Y. | DIAMOND GRINDING OF PCCP |  |
| 0140 | 502030 | 210.000 | L.F. | DRILLED SHAFT FOUNDATION 30" DIAMETER |  |
| 0150 | 502036 | 96.000 | L.F. | DRILLED SHAFT FOUNDATION 36" DIAMETER |  |
| 0160 | 502054 | 110.000 | L.F. | DRILLED SHAFT FOUNDATION 54" DIAMETER |  |
| 0170 | 506000 | 9,300.000 | S.F. | MSE PANEL WALL |  |
| 0180 | 506100 | 40.000 | C.Y. | EXCAVATION OF UNSUITABLE FOUNDATION MATERIAL |  |
| 0190 | 511000 | 250.000 | C.Y. | STRUCTURAL CONCRETE, CLASS A |  |
| 0200 | 515000 | 10.000 | C.Y. | REINF.CONCRETE FOR MINOR STRUCTURES |  |
| 0210 | 531001 | 18,500.000 | S.F. | PERMANENT ANTI-GRAFFITI PROTECTIVE COATING |  |
| 0220 | 540060 | 19,925.000 | LB | REINFORCING BARS GRADE 60 |  |
| 0230 | 547000 | 1.000 | LS | SAFETY AND ENVIRONMENTAL REQUIREMENTS |  |
| 0240 | 548002 | 9,200.000 | S.F. | COATING OF CONCRETE - PAINT |  |
| 0250 | 570437 | 1,662.000 | L.F. | 24" STORM DRAIN CULVERT PIPE |  |
| 0260 | 570441 | 3.000 | EACH | 24" STORM DRAIN CULVERT PIPE END SECTION |  |
| 0270 | 570449 | 52.000 | L.F. | 30" STORM DRAIN CULVERT PIPE |  |
| 0280 | 570453 | 1.000 | EACH | 30" STORM DRAIN CULVERT PIPE END SECTION |  |
| 0290 | 601000 | 1.000 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  |
| 0300 | 601110 | 39,200.000 | S.Y. | REMOVAL OF SURFACING |  |
| 0310 | 602000 | 35.000 | C.Y. | RIPRAP CLASS A |  |
| 0320 | 602060 | 35.000 | S.Y. | RIPRAP CLASS G |  |
| 0330 | 603100 | 11.000 | ACRE | TEMPORARY SOIL STABILANT |  |
| 0340 | 603262 | 3,800.000 | L.F. | COMPOSTED MULCH SOCKS |  |
| 0350 | 603281 | 1.000 | LS | SWPPP PLAN PREPARATION AND MAINTENANCE |  |
| 0360 | 606001 | 1,637.500 | L.F. | SINGLE FACE W-BEAM GUARDRAIL |  |
| 0370 | 606051 | 6.000 | EACH | END TREATMENT TL-3 END TERMINAL |  |
| 0380 | 606062 | 6.000 | EACH | TRANSITION METAL BARRIER TO RIGID BARRIER |  |
| 0390 | 606498 | 2.000 | EACH | POST AND CABLE BARRIER END ANCHOR |  |
| 0400 | 606542 | 834.000 | L.F. | CONCRETE WALL BARRIER 42" |  |
| 0410 | 606554 | 214.000 | L.F. | CONCRETE WALL BARRIER 54" |  |
| 0420 | 606590 | 294.000 | L.F. | CONCRETE WALL BARRIER (MODIFIED) |  |
| 0430 | 606595 | 438.000 | L.F. | CONCRETE WALL BARRIER (HALF SECTION) |  |
| 0440 | 606610 | 6,500.000 | L.F. | TCWB RETAINED BY THE CONTRACTOR (10') |  |
| 0450 | 606619 | 13,500.000 | L.F. | RESETTING OF TCWB (10') |  |
| 0460 | 607004 | 4,170.000 | L.F. | BARBED WIRE FENCE 4' |  |
| 0470 | 607015 | 17.000 | EACH | BRACES/CORNER POSTS |  |
| 0480 | 608004 | 1,470.000 | S.Y. | CONCRETE SIDEWALK 4" |  |
| 0490 | 608404 | 1,000.000 | S.Y. | CONCRETE MEDIAN PAVEMENT 4" (COLORED AND PATTERNED) |  |
| 0500 | 609424 | 4,220.000 | L.F. | CONCRETE VERTICAL CURB AND GUTTER TYPE B 6" X 24" |  |
| 0510 | 609478 | 2,610.000 | L.F. | CONCRETE VERTICAL CURB AND GUTTER TYPE D 6" X 18" |  |
| 0520 | 609636 | 20.000 | L.F. | CONCRETE VALLEY GUTTER 6" X 36" |  |
| 0530 | 610032 | 1.000 | EACH | CATTLE GUARD 32' |  |
| 0540 | 613000 | 1.000 | LS | CLEANING CULVERTS AND DRAINAGE STRUCTURES |  |
| 0550 | 618000 | 1.000 | LS | TRAFFIC CONTROL MANAGEMENT |  |
| 0560 | 621000 | 1.000 | LS | MOBILIZATION |  |
| 0570 | 622300 | 1.000 | LS | FIELD LABORATORY TESTING EQUIPMENT | $50,000.00000 |
| 0580 | 623003 | 1.000 | EACH | MEDIAN DROP INLET, TYPE I, 3' TO 6' |  |
| 0590 | 623331 | 2.000 | EACH | CURB DROP INLET TYPE I-B, OVER 4' |  |
| 0600 | 623332 | 4.000 | EACH | CURB DROP INLET TYPE II-B, OVER 4' |  |
| 0610 | 623333 | 9.000 | EACH | CURB DROP INLET TYPE III-B, OVER 4' |  |
| 0620 | 632000 | 9.000 | ACRE | CLASS A SEEDING |  |
| 0630 | 662000 | 1.000 | EACH | MANHOLE TYPE C-4' DIAMETER 0' TO 6' DEPTH |  |
| 0640 | 667110 | 5.000 | EACH | MAIL BOX INSTALLATION-SINGLE |  |
| 0650 | 667210 | 90.000 | S.Y. | LANDSCAPE GRAVEL |  |
| 0660 | 701000 | 850.000 | S.F. | PANEL SIGNS |  |
| 0670 | 701030 | 7.000 | EACH | REMOVE AND RESET PANEL SIGN |  |
| 0680 | 701040 | 2.000 | EACH | REMOVE AND RESET EXTRUDED PANEL SIGN |  |
| 0690 | 701100 | 1,740.000 | L.F. | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS |  |
| 0700 | 701109 | 80.000 | L.F. | STEEL I-BEAM POST TYPE W6X9 |  |
| 0710 | 701209 | 4.000 | EACH | BREAKAWAY BASE SYSTEM FOR STEEL I BEAM POST W6X9 |  |
| 0720 | 702000 | 2,810.000 | S.F. | CONSTRUCTION SIGNING |  |
| 0730 | 702100 | 3,680.000 | L.F. | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING |  |
| 0740 | 702101 | 6.000 | EACH | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING |  |
| 0750 | 702110 | 25.000 | EACH | PORTABLE SIGN SUPPORT |  |
| 0760 | 702238 | 24.000 | EACH | BARRICADE, TYPE III-8' |  |
| 0770 | 702525 | 280.000 | EACH | CHANNELIZATION DEVICES TYPE DRUM |  |
| 0780 | 702600 | 2.000 | EACH | SEQUENTIAL ARROW DISPLAY |  |
| 0790 | 702610 | 3.000 | EACH | PORTABLE CHANGEABLE MESSAGE SIGN |  |
| 0800 | 702700 | 1.000 | LS | TEMPORARY SIGNAL SPAN |  |
| 0810 | 702811 | 1.000 | LS | TRAFFIC CONTROL DEVICES FOR PEDESTRIAN AND BICYCLIST |  |
| 0820 | 702850 | 1.000 | ALOW | LAW ENFORCEMENT IN CONSTRUCTION ZONE | $30,000.00000 |
| 0830 | 703001 | 6.000 | EACH | OBJECT MARKER TYPE 1 |  |
| 0840 | 704000 | 25,300.000 | L.F. | RETROREFLECTORIZED PAINTED MARKINGS 4" |  |
| 0850 | 704099 | 111,200.000 | L.F. | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" |  |
| 0860 | 704100 | 36,900.000 | L.F. | REMOVABLE MARKING TAPE 4" |  |
| 0870 | 704101 | 16.000 | EACH | TEMPORARY WORD OR SYMBOL |  |
| 0880 | 704700 | 9,300.000 | L.F. | HOT THERMOPLASTIC PAVEMENT MARKINGS 4" |  |
| 0890 | 704704 | 700.000 | L.F. | HOT THERMOPLASTIC PAVEMENT MARKING 24" |  |
| 0900 | 704706 | 5,405.000 | L.F. | HOT THERMOPLASTIC PAVEMENT MARKINGS 12" |  |
| 0910 | 704715 | 4.000 | EACH | HOT THERMOPLASTIC PAVEMENT MARKING COMBINATION (THRU AND RIGHT) ARROW |  |
| 0920 | 704717 | 4.000 | EACH | HOT THERMOPLASTIC PAVEMENT MARKING RIGHT ARROW |  |
| 0930 | 704718 | 14.000 | EACH | HOT THERMOPLASTIC PAVEMENT MARKING LEFT ARROW |  |
| 0940 | 704720 | 10.000 | EACH | HOT THERMOPLASTIC PAVEMENT MARKING WORD (ONLY) |  |
| 0950 | 704728 | 16.000 | L.F. | HOT THERMOPLASTIC PAVEMENT MARKING YIELD LINE |  |
| 0960 | 704731 | 9.000 | EACH | HOT THERMOPLASTIC MARKING LANE SYMBOL (BIKEWAY) |  |
| 0970 | 704735 | 4.000 | EACH | HOT THERMOPLASTIC PAVEMENT MARKING RIGHT LANE DROP ARROW |  |
| 0980 | 704869 | 85.000 | EACH | PLOWABLE REFLECTIVE RAISED PAVEMENT MARKER TYPE PG |  |
| 0990 | 706130 | 2.000 | EACH | SERVICE RISER (COMBINATION) |  |
| 1000 | 706230 | 4.000 | EACH | METER PEDESTAL (COMBINATION) |  |
| 1010 | 706240 | 2.000 | EACH | UNINTERRUPTED POWER SUPPLY (UPS) |  |
| 1020 | 706350 | 1.000 | LS | POWER SERVICE INSTALLATION | $20,000.00000 |
| 1030 | 706405 | 4.000 | EACH | LIGHTING CONTROL CABINET-SIX CIRCUIT |  |
| 1040 | 707010 | 8.000 | EACH | TYPE I STANDARD, 10' |  |
| 1050 | 707013 | 1.000 | EACH | TYPE I STANDARD, 13' |  |
| 1060 | 707015 | 5.000 | EACH | TYPE I STANDARD, 15' |  |
| 1070 | 707320 | 1.000 | EACH | TYPE III STANDARD, 20' ARM |  |
| 1080 | 707325 | 1.000 | EACH | TYPE III STANDARD, 25' ARM |  |
| 1090 | 707330 | 2.000 | EACH | TYPE III STANDARD, 30' ARM |  |
| 1100 | 707335 | 2.000 | EACH | TYPE III STANDARD, 35' ARM |  |
| 1110 | 707540 | 27.000 | EACH | TYPE V STANDARD, 40' |  |
| 1120 | 707620 | 6.000 | EACH | TYPE VI STANDARD, 120' |  |
| 1130 | 707670 | 6.000 | EACH | HIGH MAST LOWERING DEVICE |  |
| 1140 | 709020 | 16,445.000 | L.F. | RIGID ELECTRICAL CONDUIT 2" (DIA.) |  |
| 1150 | 709030 | 2,120.000 | L.F. | RIGID ELECTRICAL CONDUIT 3" (DIA.) |  |
| 1160 | 709040 | 480.000 | L.F. | RIGID ELECTRICAL CONDUIT 4" (DIA.) |  |
| 1170 | 710000 | 33.000 | EACH | ELECTRICAL PULL BOX (STANDARD) |  |
| 1180 | 710010 | 33.000 | EACH | ELECTRICAL PULL BOX (LARGE) |  |
| 1190 | 710400 | 2.000 | EACH | TRAFFIC SIGNAL MANHOLE |  |
| 1200 | 711005 | 935.000 | L.F. | MULTI CONDUCTOR CABLE 5 |  |
| 1210 | 711007 | 2,385.000 | L.F. | MULTI CONDUCTOR CABLE 7 |  |
| 1220 | 711020 | 2,500.000 | L.F. | MULTI CONDUCTOR CABLE 20 |  |
| 1230 | 711102 | 27,560.000 | L.F. | SINGLE CONDUCTOR 2 |  |
| 1240 | 711106 | 3,800.000 | L.F. | SINGLE CONDUCTOR 6 |  |
| 1250 | 711210 | 470.000 | L.F. | SINGLE CONDUCTOR 1/0 |  |
| 1260 | 711512 | 655.000 | L.F. | COMMUNICATION CABLE 12 PAIR |  |
| 1270 | 712011 | 2.000 | EACH | 1 SECTION TRAFFIC SIGNAL ASSEMBLY (LED) |  |
| 1280 | 712031 | 16.000 | EACH | 3 SECTION TRAFFIC SIGNAL ASSEMBLY (LED) |  |
| 1290 | 712041 | 4.000 | EACH | 4 SECTION TRAFFIC SIGNAL ASSEMBLY (LED) |  |
| 1300 | 712202 | 15.000 | EACH | PEDESTRIAN COUNTDOWN SIGNAL (LED) |  |
| 1310 | 712330 | 10.000 | EACH | 3 SECTION BACKPLATE |  |
| 1320 | 713025 | 15.000 | EACH | ACCESSIBLE PEDESTRIAN SIGNAL PUSH BUTTON STATION |  |
| 1330 | 713430 | 2.000 | EACH | PHASE SELECTOR MODULE |  |
| 1340 | 713511 | 6.000 | EACH | OPTICAL DETECTOR, 1 DIRECTION, 1 CHANNEL |  |
| 1350 | 713600 | 1,610.000 | L.F. | OPTICAL DETECTOR CABLE |  |
| 1360 | 713826 | 6.000 | EACH | RADAR PRESENCE DETECTOR |  |
| 1370 | 713842 | 1,520.000 | L.F. | RADAR DETECTOR CABLE |  |
| 1380 | 713843 | 2.000 | EACH | RADAR DETECTION CABINET INTERFACE UNIT |  |
| 1390 | 714000 | 2.000 | EACH | TRAFFIC ACTUATED CONTROLLER |  |
| 1400 | 714100 | 1.000 | EACH | SYSTEM MASTER |  |
| 1410 | 714280 | 2.000 | EACH | 8 PHASE DOUBLE RING CONTROLLER CABINET |  |
| 1420 | 714300 | 1.000 | LS | CLOSED LOOP TRAFFIC CONTROL SYSTEM |  |
| 1430 | 715000 | 1.000 | EACH | BEACON ASSEMBLY |  |
| 1440 | 716701 | 27.000 | EACH | LED ROADWAY LUMINAIRE |  |
| 1450 | 716702 | 24.000 | EACH | LED HIGH MAST LUMINAIRE |  |
| 1460 | 720050 | 3.000 | EACH | PERMANENT VEHICULAR IMPACT ATTENUATOR UNIT |  |
| 1470 | 720060 | 8.000 | EACH | VEHICULAR IMPACT ATTENUATOR UNIT-WORK ZONES |  |
| 1480 | 720110 | 23.000 | EACH | REMOVE/RESET IMPACT ATTENUATOR UNIT |  |
| 1490 | 721000 | 43,500.000 | L.F. | REMOVAL OF PAVEMENT MARKING |  |
| 1500 | 721101 | 3.000 | EACH | REMOVAL OF PAVEMENT MARKING SYMBOL |  |
| 1510 | 801000 | 1.000 | LS | CONSTRUCTION STAKING BY THE CONTRACTOR |  |
| 1520 | 802000 | 1.000 | LS | POST CONSTRUCTION PLANS | $7,500.00000 |
| 1530 | 803000 | 1.000 | LS | SCHEDULE SOFTWARE |  |
| 1540 | 803020 | 1.000 | LS | CPM HARDWARE/EQUIPMENT |  |
| **Section 0002: BRIDGE** | | | | | |
| 1550 | 210002 | 175.000 | C.Y. | MAJOR STRUCTURE EXCAVATION |  |
| 1560 | 210003 | 2,100.000 | C.Y. | MAJOR STRUCTURE BACKFILL |  |
| 1570 | 502048 | 1,155.000 | L.F. | DRILLED SHAFT FOUNDATION 48" DIAMETER |  |
| 1580 | 502600 | 3.000 | L.F. | OBSTRUCTION REMOVAL |  |
| 1590 | 505001 | 24.000 | EACH | CROSSHOLE SONIC LOGGING DEPARTMENT TESTING |  |
| 1600 | 505010 | 3.000 | EACH | LOW STRAIN INTEGRITY DEPARTMENT TESTING |  |
| 1610 | 511000 | 540.000 | C.Y. | STRUCTURAL CONCRETE, CLASS A |  |
| 1620 | 511070 | 1,110.000 | C.Y. | STRUCTURAL CONCRETE, CLASS HPD |  |
| 1630 | 511200 | 200.000 | S.Y. | STRUCTURAL CONCRETE, CLASS A-4" |  |
| 1640 | 514042 | 438.000 | L.F. | CONCRETE BARRIER RAILINGS 42" |  |
| 1650 | 515000 | 10.000 | C.Y. | REINF.CONCRETE FOR MINOR STRUCTURES |  |
| 1660 | 518054 | 1,980.000 | L.F. | PRESTRESSED CONCRETE BRIDGE MEMBER TYPE 54 |  |
| 1670 | 531001 | 11,800.000 | S.F. | PERMANENT ANTI-GRAFFITI PROTECTIVE COATING |  |
| 1680 | 540060 | 230,600.000 | LB | REINFORCING BARS GRADE 60 |  |
| 1690 | 540160 | 211,000.000 | LB | EPOXY COATED REINFORCING BARS GRADE 60 |  |
| 1700 | 541000 | 20,160.000 | LB | STRUCTURAL STEEL FOR CONCRETE BRIDGES |  |
| 1710 | 548001 | 11,800.000 | S.F. | COATING OF CONCRETE - STAIN |  |
| 1720 | 560000 | 44.000 | EACH | ELASTOMERIC BEARING PADS |  |
| 1730 | 562000 | 198.000 | L.F. | BRIDGE JOINT STRIP SEAL |  |
| 1740 | 563099 | 194.000 | L.F. | POLYMER BRIDGE JOINT SEALS |  |
| 1750 | 565000 | 247.000 | L.F. | PREFORMED SILICONE-COATED FOAM JOINT SYSTEM |  |
| 1760 | 601000 | 1.000 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  |
| 1770 | 604300 | 670.000 | S.Y. | GEOGRID REINFORCEMENT |  |
| 1780 | 607076 | 440.000 | L.F. | PEDESTRIAN SCREENING FENCE, TYPE 1 |  |
| 1790 | 709040 | 220.000 | L.F. | RIGID ELECTRICAL CONDUIT 4" (DIA.) |  |

|  |  |  |
| --- | --- | --- |
|  | **Proposal 2104340** |  |

Roadway Rehabilitation

|  |  |  |  |
| --- | --- | --- | --- |
| Proposal information table | | | |
| **Date Generated:** | 07/22/2020 | **Sections:** | 1 |
| **Date Revised:** |  | **Amendments:** | 0 |
| **Call Order:** | 003 | **Highway Number:** |  |
| **Items:** | 29 | **Counties:** | Eddy Lea |
| **Project ID:** | 2104340 |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Proposal items table | | | | | |
| **Line** | **Item** | **Quantity** | **Unit** | **Description** | **Price** |
| **Section 0001: ROADWAY** | | | | | |
| 0010 | 301012 | 259,570.000 | S.Y. | FULL DEPTH RECLAMATION - FOAMED ASPHALT STABILIZED BASE |  |
| 0020 | 301014 | 3,736.000 | TON | ASPHALT BINDER |  |
| 0030 | 301015 | 1,602.000 | TON | MINERAL FILLER |  |
| 0040 | 303130 | 1,160.000 | S.Y. | BASE COURSE 3" |  |
| 0050 | 403715 | 8,770.000 | TON | RUBBERIZED OPEN-GRADED FRICTION COURSE COMPLETE |  |
| 0060 | 407000 | 235.000 | TON | ASPHALT MATERIAL FOR TACK COAT |  |
| 0070 | 414000 | 484,900.000 | SYIN | COLD MILLING (ASPHALT) |  |
| 0080 | 416004 | 440.000 | S.Y. | MINOR PAVEMENT HMA SP-IV |  |
| 0090 | 423283 | 67,760.000 | TON | HMA SP-IV COMPLETE |  |
| 0100 | 601000 | 1.000 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  |
| 0110 | 618000 | 1.000 | LS | TRAFFIC CONTROL MANAGEMENT |  |
| 0120 | 621000 | 1.000 | LS | MOBILIZATION |  |
| 0130 | 631000 | 180,600.000 | L.F. | RUMBLE STRIPS |  |
| 0140 | 701000 | 1,550.000 | S.F. | PANEL SIGNS |  |
| 0150 | 701100 | 2,900.000 | L.F. | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS |  |
| 0160 | 702000 | 675.000 | S.F. | CONSTRUCTION SIGNING |  |
| 0170 | 702100 | 518.000 | L.F. | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING |  |
| 0180 | 702110 | 34.000 | EACH | PORTABLE SIGN SUPPORT |  |
| 0190 | 702238 | 1.000 | EACH | BARRICADE, TYPE III-8' |  |
| 0200 | 702525 | 262.000 | EACH | CHANNELIZATION DEVICES TYPE DRUM |  |
| 0210 | 702610 | 5.000 | EACH | PORTABLE CHANGEABLE MESSAGE SIGN |  |
| 0220 | 704000 | 804,000.000 | L.F. | RETROREFLECTORIZED PAINTED MARKINGS 4" |  |
| 0230 | 704099 | 244,000.000 | L.F. | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" |  |
| 0240 | 704875 | 3,395.000 | EACH | TEMPORARY REFLECTIVE RAISED PAVEMENT MARKER, TYPE TD |  |
| 0250 | 704876 | 4,625.000 | EACH | TEMPORARY REFLECTIVE RAISED PAVEMENT MARKER, TYPE TG |  |
| 0260 | 801000 | 1.000 | LS | CONSTRUCTION STAKING BY THE CONTRACTOR |  |
| 0270 | 802000 | 1.000 | LS | POST CONSTRUCTION PLANS | $5,000.00000 |
| 0280 | 803000 | 1.000 | LS | SCHEDULE SOFTWARE |  |
| 0290 | 803020 | 1.000 | LS | CPM HARDWARE/EQUIPMENT |  |

|  |  |
| --- | --- |
| **Proposal 1101560** |  |

Roadway Recon/Rehab, Bridge Rpl, Lighting

|  |  |  |  |
| --- | --- | --- | --- |
| Proposal information table | | | |
| **Date Generated:** | 07/22/2020 | **Sections:** | 2 |
| **Date Revised:** |  | **Amendments:** | 0 |
| **Call Order:** | 004 | **Highway Number:** |  |
| **Items:** | 91 | **Counties:** | Hidalgo |
| **Project ID:** | 1101560 |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Proposal items table | | | | | |
| **Line** | **Item** | **Quantity** | **Unit** | **Description** | **Price** |
| **Section 0001: ROADWAY** | | | | | |
| 0010 | 201000 | 1.000 | LS | CLEARING AND GRUBBING |  |
| 0020 | 203000 | 19,740.000 | C.Y. | UNCLASSIFIED EXCAVATION |  |
| 0030 | 203100 | 1,180.000 | C.Y. | BORROW |  |
| 0040 | 203211 | 4,100.000 | S.Y. | UNSTABLE SUBGRADE STABILIZATION |  |
| 0050 | 207000 | 20,500.000 | S.Y. | SUBGRADE PREPARATION |  |
| 0060 | 209000 | 1.000 | MILE | BLADING AND RESHAPING |  |
| 0070 | 303000 | 15,440.000 | TON | BASE COURSE |  |
| 0080 | 403715 | 500.000 | TON | RUBBERIZED OPEN-GRADED FRICTION COURSE COMPLETE |  |
| 0090 | 405000 | 14,220.000 | S.Y. | DETOUR PAVEMENT CONSTRUCTION |  |
| 0100 | 407000 | 6.000 | TON | ASPHALT MATERIAL FOR TACK COAT |  |
| 0110 | 408100 | 40.000 | TON | PRIME COAT MATERIAL |  |
| 0120 | 414130 | 474.000 | S.Y. | COLD MILLING (ASPHALT) 3" |  |
| 0130 | 416014 | 10,950.000 | TON | MINOR PAVEMENT HMA SP-IV |  |
| 0140 | 502030 | 160.000 | L.F. | DRILLED SHAFT FOUNDATION 30" DIAMETER |  |
| 0150 | 540060 | 4,800.000 | LB | REINFORCING BARS GRADE 60 |  |
| 0160 | 601000 | 1.000 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  |
| 0170 | 601110 | 16,970.000 | S.Y. | REMOVAL OF SURFACING |  |
| 0180 | 603100 | 16.000 | ACRE | TEMPORARY SOIL STABILANT |  |
| 0190 | 604310 | 45,200.000 | S.Y. | GEOGRID BASE REINFORCEMENT |  |
| 0200 | 606001 | 975.000 | L.F. | SINGLE FACE W-BEAM GUARDRAIL |  |
| 0210 | 606051 | 4.000 | EACH | END TREATMENT TL-3 END TERMINAL |  |
| 0220 | 606062 | 4.000 | EACH | TRANSITION METAL BARRIER TO RIGID BARRIER |  |
| 0230 | 606598 | 6,200.000 | L.F. | TCWB RETAINED BY THE CONTRACTOR |  |
| 0240 | 606599 | 6,200.000 | L.F. | RESETTING OF TCWB |  |
| 0250 | 608004 | 80.000 | S.Y. | CONCRETE SIDEWALK 4" |  |
| 0260 | 608206 | 180.000 | S.Y. | CONCRETE MEDIAN PAVEMENT 6" |  |
| 0270 | 609330 | 350.000 | L.F. | CONCRETE SLOPED CURB AND GUTTER 6" X 30" |  |
| 0280 | 609430 | 960.000 | L.F. | CONCRETE VERTICAL CURB AND GUTTER TYPE B 6" X 30" |  |
| 0290 | 609706 | 70.000 | L.F. | CONCRETE LAYDOWN CURB 6" |  |
| 0300 | 617003 | 1.000 | LS | VIDEO RECORDING |  |
| 0310 | 618000 | 1.000 | LS | TRAFFIC CONTROL MANAGEMENT |  |
| 0320 | 618011 | 1.000 | LS | PUBLIC AWARENESS | $5,000.00000 |
| 0330 | 621000 | 1.000 | LS | MOBILIZATION |  |
| 0340 | 622100 | 1.000 | EACH | SUPPLEMENTAL FIELD LABORATORY |  |
| 0350 | 630100 | 6,000.000 | L.F. | MULTIPLE GLARE SHIELDING 24 IN |  |
| 0360 | 631000 | 5,815.000 | L.F. | RUMBLE STRIPS |  |
| 0370 | 632000 | 13.000 | ACRE | CLASS A SEEDING |  |
| 0380 | 701000 | 270.000 | S.F. | PANEL SIGNS |  |
| 0390 | 701100 | 630.000 | L.F. | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS |  |
| 0400 | 702000 | 2,076.000 | S.F. | CONSTRUCTION SIGNING |  |
| 0410 | 702100 | 1,890.000 | L.F. | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING |  |
| 0420 | 702101 | 12.000 | EACH | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING |  |
| 0430 | 702110 | 90.000 | EACH | PORTABLE SIGN SUPPORT |  |
| 0440 | 702238 | 12.000 | EACH | BARRICADE, TYPE III-8' |  |
| 0450 | 702525 | 250.000 | EACH | CHANNELIZATION DEVICES TYPE DRUM |  |
| 0460 | 702600 | 2.000 | EACH | SEQUENTIAL ARROW DISPLAY |  |
| 0470 | 702610 | 5.000 | EACH | PORTABLE CHANGEABLE MESSAGE SIGN |  |
| 0480 | 704000 | 5,800.000 | L.F. | RETROREFLECTORIZED PAINTED MARKINGS 4" |  |
| 0490 | 704099 | 58,000.000 | L.F. | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" |  |
| 0500 | 704701 | 20,900.000 | L.F. | HOT THERMOPLASTIC PAVEMENT MARKINGS 6" |  |
| 0510 | 704718 | 3.000 | EACH | HOT THERMOPLASTIC PAVEMENT MARKING LEFT ARROW |  |
| 0520 | 704869 | 70.000 | EACH | PLOWABLE REFLECTIVE RAISED PAVEMENT MARKER TYPE PG |  |
| 0530 | 704876 | 862.000 | EACH | TEMPORARY REFLECTIVE RAISED PAVEMENT MARKER, TYPE TG |  |
| 0540 | 704877 | 898.000 | EACH | TEMPORARY REFLECTIVE RAISED PAVEMENT MARKER, TYPE TH |  |
| 0550 | 705000 | 1.000 | ALOW | SIGNAL/LIGHTING SYSTEM START-UP COSTS | $5,000.00000 |
| 0560 | 706010 | 1.000 | EACH | SERVICE POLE (LIGHTING) |  |
| 0570 | 706110 | 1.000 | EACH | SERVICE RISER (LIGHTING) |  |
| 0580 | 706350 | 1.000 | LS | POWER SERVICE INSTALLATION | $3,500.00000 |
| 0590 | 706420 | 1.000 | EACH | LIGHTING CONTROL CABINET-TWO CIRCUIT |  |
| 0600 | 707540 | 20.000 | EACH | TYPE V STANDARD, 40' |  |
| 0610 | 709020 | 6,265.000 | L.F. | RIGID ELECTRICAL CONDUIT 2" (DIA.) |  |
| 0620 | 709030 | 25.000 | L.F. | RIGID ELECTRICAL CONDUIT 3" (DIA.) |  |
| 0630 | 710000 | 27.000 | EACH | ELECTRICAL PULL BOX (STANDARD) |  |
| 0640 | 711102 | 12,605.000 | L.F. | SINGLE CONDUCTOR 2 |  |
| 0650 | 716400 | 2.000 | EACH | UNDERPASS LUMINAIRE |  |
| 0660 | 716701 | 20.000 | EACH | LED ROADWAY LUMINAIRE |  |
| 0670 | 720060 | 2.000 | EACH | VEHICULAR IMPACT ATTENUATOR UNIT-WORK ZONES |  |
| 0680 | 720110 | 2.000 | EACH | REMOVE/RESET IMPACT ATTENUATOR UNIT |  |
| 0690 | 721000 | 24,610.000 | L.F. | REMOVAL OF PAVEMENT MARKING |  |
| 0700 | 801000 | 1.000 | LS | CONSTRUCTION STAKING BY THE CONTRACTOR |  |
| 0710 | 802000 | 1.000 | LS | POST CONSTRUCTION PLANS | $5,000.00000 |
| 0720 | 803000 | 1.000 | LS | SCHEDULE SOFTWARE |  |
| 0730 | 803020 | 1.000 | LS | CPM HARDWARE/EQUIPMENT |  |
| **Section 0002: BRIDGE** | | | | | |
| 0740 | 210002 | 4,510.000 | C.Y. | MAJOR STRUCTURE EXCAVATION |  |
| 0750 | 210003 | 5,500.000 | C.Y. | MAJOR STRUCTURE BACKFILL |  |
| 0760 | 511000 | 1,016.000 | C.Y. | STRUCTURAL CONCRETE, CLASS A |  |
| 0770 | 511070 | 713.000 | C.Y. | STRUCTURAL CONCRETE, CLASS HPD |  |
| 0780 | 511200 | 2,148.000 | S.Y. | STRUCTURAL CONCRETE, CLASS A-4" |  |
| 0790 | 514042 | 556.000 | L.F. | CONCRETE BARRIER RAILINGS 42" |  |
| 0800 | 518045 | 876.000 | L.F. | PRESTRESSED CONCRETE BRIDGE MEMBER TYPE 45 |  |
| 0810 | 540060 | 95,400.000 | LB | REINFORCING BARS GRADE 60 |  |
| 0820 | 540160 | 171,500.000 | LB | EPOXY COATED REINFORCING BARS GRADE 60 |  |
| 0830 | 541000 | 9,420.000 | LB | STRUCTURAL STEEL FOR CONCRETE BRIDGES |  |
| 0840 | 560000 | 24.000 | EACH | ELASTOMERIC BEARING PADS |  |
| 0850 | 562000 | 202.000 | L.F. | BRIDGE JOINT STRIP SEAL |  |
| 0860 | 565000 | 494.000 | L.F. | PREFORMED SILICONE-COATED FOAM JOINT SYSTEM |  |
| 0870 | 601000 | 1.000 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  |
| 0880 | 601995 | 2,200.000 | L.F. | AC-ABATEMENT |  |
| 0890 | 604002 | 1,630.000 | S.Y. | GEOTEXTILE CLASS 2 |  |
| 0900 | 604300 | 5,732.000 | S.Y. | GEOGRID REINFORCEMENT |  |
| 0910 | 606532 | 300.000 | L.F. | CONCRETE WALL BARRIER 32" |  |

|  |  |  |
| --- | --- | --- |
|  | **Proposal 5101291** |  |

Bridge Rehabilitation, Roadway Rehabilitation

|  |  |  |  |
| --- | --- | --- | --- |
| Proposal information table | | | |
| **Date Generated:** | 07/22/2020 | **Sections:** | 2 |
| **Date Revised:** |  | **Amendments:** | 0 |
| **Call Order:** | 005 | **Highway Number:** |  |
| **Items:** | 68 | **Counties:** | Rio Arriba |
| **Project ID:** | 5101291 |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Proposal items table | | | | | |
| **Line** | **Item** | **Quantity** | **Unit** | **Description** | **Price** |
| **Section 0001: BRIDGE** | | | | | |
| 0010 | 210002 | 422.000 | C.Y. | MAJOR STRUCTURE EXCAVATION |  |
| 0020 | 210003 | 319.000 | C.Y. | MAJOR STRUCTURE BACKFILL |  |
| 0030 | 411000 | 4.000 | LB | HOT POURED CRACK SEALING |  |
| 0040 | 453000 | 450.000 | LB | VOID FILLING OR SLAB JACKING AT STRUCTURE GRADE |  |
| 0050 | 511070 | 92.000 | C.Y. | STRUCTURAL CONCRETE, CLASS HPD |  |
| 0060 | 514042 | 88.000 | L.F. | CONCRETE BARRIER RAILINGS 42" |  |
| 0070 | 533000 | 75.000 | S.Y. | REPAIR OF CONCRETE STRUCTURES |  |
| 0080 | 533001 | 26.000 | EACH | EMBEDDED GALVANIC ANODES |  |
| 0090 | 533003 | 100.000 | LB | REPLACEMENT REINFORCING BARS |  |
| 0100 | 536001 | 1,573.000 | S.Y. | EPOXY URETHANE POLYMER CONCRETE BRIDGE DECK OVERLAY |  |
| 0110 | 540076 | 14,700.000 | LB | UNCOATED CORROSION RESISTANT REINFORCING BARS GRADE 75 |  |
| 0120 | 562000 | 93.000 | L.F. | BRIDGE JOINT STRIP SEAL |  |
| 0130 | 563099 | 148.000 | L.F. | POLYMER BRIDGE JOINT SEALS |  |
| 0140 | 601000 | 1.000 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  |
| 0150 | 602100 | 58.000 | C.Y. | SACKED CONCRETE REVETMENT |  |
| 0160 | 604300 | 604.000 | S.Y. | GEOGRID REINFORCEMENT |  |
| **Section 0002: ROADWAY** | | | | | |
| 0170 | 201000 | 1.000 | LS | CLEARING AND GRUBBING |  |
| 0180 | 403600 | 870.000 | S.Y. | OPEN GRADED FRICTION COURSE COMPLETE |  |
| 0190 | 407000 | 2.000 | TON | ASPHALT MATERIAL FOR TACK COAT |  |
| 0200 | 408100 | 1.000 | TON | PRIME COAT MATERIAL |  |
| 0210 | 414000 | 5,000.000 | SYIN | COLD MILLING (ASPHALT) |  |
| 0220 | 416003 | 1,460.000 | S.Y. | MINOR PAVEMENT HMA SP-III |  |
| 0230 | 502024 | 1,230.000 | L.F. | DRILLED SHAFT FOUNDATION 24" DIAMETER |  |
| 0240 | 502300 | 91,020.000 | LB | STEEL SHAPE REINFORCEMENT |  |
| 0250 | 515000 | 20.000 | C.Y. | REINF.CONCRETE FOR MINOR STRUCTURES |  |
| 0260 | 570012 | 310.000 | L.F. | 12" CULVERT PIPE |  |
| 0270 | 570024 | 210.000 | L.F. | 24" CULVERT PIPE |  |
| 0280 | 570025 | 1.000 | EACH | 24" CULVERT PIPE END SECTION |  |
| 0290 | 601000 | 1.000 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  |
| 0300 | 601110 | 100.000 | S.Y. | REMOVAL OF SURFACING |  |
| 0310 | 602000 | 280.000 | C.Y. | RIPRAP CLASS A |  |
| 0320 | 602060 | 530.000 | S.Y. | RIPRAP CLASS G |  |
| 0330 | 603100 | 2.000 | ACRE | TEMPORARY SOIL STABILANT |  |
| 0340 | 603262 | 1,020.000 | L.F. | COMPOSTED MULCH SOCKS |  |
| 0350 | 603281 | 1.000 | LS | SWPPP PLAN PREPARATION AND MAINTENANCE |  |
| 0360 | 606001 | 675.000 | L.F. | SINGLE FACE W-BEAM GUARDRAIL |  |
| 0370 | 606051 | 2.000 | EACH | END TREATMENT TL-3 END TERMINAL |  |
| 0380 | 606062 | 2.000 | EACH | TRANSITION METAL BARRIER TO RIGID BARRIER |  |
| 0390 | 606532 | 180.000 | L.F. | CONCRETE WALL BARRIER 32" |  |
| 0400 | 606542 | 20.000 | L.F. | CONCRETE WALL BARRIER 42" |  |
| 0410 | 606710 | 960.000 | L.F. | TCWB RETAINED BY THE CONTRACTOR (20') |  |
| 0420 | 606719 | 960.000 | L.F. | RESETTING OF TCWB (20') |  |
| 0430 | 607010 | 330.000 | L.F. | BARBED WIRE FENCE (GAME FENCE) 4' |  |
| 0440 | 607199 | 200.000 | L.F. | REMOVE AND REBUILD FENCE |  |
| 0450 | 618000 | 1.000 | LS | TRAFFIC CONTROL MANAGEMENT |  |
| 0460 | 621000 | 1.000 | LS | MOBILIZATION |  |
| 0470 | 623001 | 1.000 | EACH | MEDIAN DROP INLET TYPE I (URBAN) H=3'1" TO 6'0" |  |
| 0480 | 623410 | 3.000 | EACH | DROP INLET SPECIAL DESIGN |  |
| 0490 | 631000 | 600.000 | L.F. | RUMBLE STRIPS |  |
| 0500 | 632000 | 1.000 | ACRE | CLASS A SEEDING |  |
| 0510 | 632020 | 1.000 | ACRE | CLASS C SEEDING |  |
| 0520 | 702000 | 100.000 | S.F. | CONSTRUCTION SIGNING |  |
| 0530 | 702100 | 70.000 | L.F. | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING |  |
| 0540 | 702101 | 6.000 | EACH | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING |  |
| 0550 | 702599 | 200.000 | L.F. | TEMPORARY PORTABLE RUMBLE STRIPS |  |
| 0560 | 702610 | 2.000 | EACH | PORTABLE CHANGEABLE MESSAGE SIGN |  |
| 0570 | 702612 | 2.000 | EACH | PORTABLE FLOODLIGHT SYSTEM |  |
| 0580 | 702710 | 1.000 | EACH | MOBILE TRAFFIC SIGNAL SYSTEM |  |
| 0590 | 702810 | 1.000 | LS | TRAFFIC CONTROL DEVICES FOR CONSTRUCTION |  |
| 0600 | 704000 | 9,550.000 | L.F. | RETROREFLECTORIZED PAINTED MARKINGS 4" |  |
| 0610 | 704100 | 1,200.000 | L.F. | REMOVABLE MARKING TAPE 4" |  |
| 0620 | 720060 | 2.000 | EACH | VEHICULAR IMPACT ATTENUATOR UNIT-WORK ZONES |  |
| 0630 | 720110 | 2.000 | EACH | REMOVE/RESET IMPACT ATTENUATOR UNIT |  |
| 0640 | 721000 | 460.000 | L.F. | REMOVAL OF PAVEMENT MARKING |  |
| 0650 | 801000 | 1.000 | LS | CONSTRUCTION STAKING BY THE CONTRACTOR |  |
| 0660 | 802000 | 1.000 | LS | POST CONSTRUCTION PLANS | $10,000.00000 |
| 0670 | 803000 | 1.000 | LS | SCHEDULE SOFTWARE |  |
| 0680 | 803020 | 1.000 | LS | CPM HARDWARE/EQUIPMENT |  |

|  |  |  |
| --- | --- | --- |
|  | **Proposal A302190** |  |

Intelligent Transportation System (ITS)

|  |  |  |  |
| --- | --- | --- | --- |
| Proposal information table | | | |
| **Date Generated:** | 07/22/2020 | **Sections:** | 1 |
| **Date Revised:** |  | **Amendments:** | 0 |
| **Call Order:** | 006 | **Highway Number:** |  |
| **Items:** | 31 | **Counties:** | Bernalillo |
| **Project ID:** | A302190 |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Proposal items table | | | | | |
| **Line** | **Item** | **Quantity** | **Unit** | **Description** | **Price** |
| **Section 0001: ROADWAY** | | | | | |
| 0010 | 201000 | 1.000 | LS | CLEARING AND GRUBBING |  |
| 0020 | 502048 | 46.000 | L.F. | DRILLED SHAFT FOUNDATION 48" DIAMETER |  |
| 0030 | 502066 | 39.000 | L.F. | DRILLED SHAFT FOUNDATION 66" DIAMETER |  |
| 0040 | 601000 | 1.000 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  |
| 0050 | 606001 | 287.500 | L.F. | SINGLE FACE W-BEAM GUARDRAIL |  |
| 0060 | 606051 | 3.000 | EACH | END TREATMENT TL-3 END TERMINAL |  |
| 0070 | 606055 | 2.000 | EACH | END TREATMENT DRIVEWAY END ANCHOR |  |
| 0080 | 618000 | 1.000 | LS | TRAFFIC CONTROL MANAGEMENT |  |
| 0090 | 621000 | 1.000 | LS | MOBILIZATION |  |
| 0100 | 701112 | 80.000 | L.F. | STEEL I-BEAM POST TYPE W6X12 |  |
| 0110 | 701212 | 6.000 | EACH | BREAKAWAY BASE SYSTEM FOR STEEL I BEAM POST W6X12 |  |
| 0120 | 701340 | 2.000 | EACH | OVERHEAD SIGN STRUCTURE, BUTTERFLY TYPE, 20-INCH |  |
| 0130 | 701343 | 1.000 | EACH | OVERHEAD SIGN STRUCTURE, BUTTERFLY TYPE, 36-INCH |  |
| 0140 | 702610 | 2.000 | EACH | PORTABLE CHANGEABLE MESSAGE SIGN |  |
| 0150 | 702810 | 1.000 | LS | TRAFFIC CONTROL DEVICES FOR CONSTRUCTION |  |
| 0160 | 702811 | 1.000 | LS | TRAFFIC CONTROL DEVICES FOR PEDESTRIAN AND BICYCLIST |  |
| 0170 | 702850 | 1.000 | ALOW | LAW ENFORCEMENT IN CONSTRUCTION ZONE | $2,500.00000 |
| 0180 | 706100 | 4.000 | EACH | SERVICE RISER (SIGNAL) |  |
| 0190 | 706200 | 6.000 | EACH | METER PEDESTAL (SIGNAL) |  |
| 0200 | 706350 | 1.000 | LS | POWER SERVICE INSTALLATION | $8,000.00000 |
| 0210 | 709020 | 16,640.000 | L.F. | RIGID ELECTRICAL CONDUIT 2" (DIA.) |  |
| 0220 | 710000 | 20.000 | EACH | ELECTRICAL PULL BOX (STANDARD) |  |
| 0230 | 711220 | 66,930.000 | L.F. | SINGLE CONDUCTOR 2/0 |  |
| 0240 | 720050 | 1.000 | EACH | PERMANENT VEHICULAR IMPACT ATTENUATOR UNIT |  |
| 0250 | 750000 | 1.000 | LS | INTELLIGENT TRANSPORTATION SYSTEM |  |
| 0260 | 750060 | 28.000 | EACH | ITS PULLBOX (33"X24"X24") |  |
| 0270 | 750100 | 12.000 | EACH | CLOSED CIRCUIT TELEVISION SYSTEM (CCTV) |  |
| 0280 | 750110 | 12.000 | EACH | CAMERA LOWERING DEVICE |  |
| 0290 | 750130 | 1.000 | EACH | ITS STEEL POLE, 30 FT |  |
| 0300 | 750150 | 11.000 | EACH | ITS STEEL POLE, 50 FT |  |
| 0310 | 801000 | 1.000 | LS | CONSTRUCTION STAKING BY THE CONTRACTOR |  |

|  |  |  |
| --- | --- | --- |
|  | **Proposal 6100841** |  |

Bridge Rehabilitation, Roadway Rehabilitation

|  |  |  |  |
| --- | --- | --- | --- |
| Proposal information table | | | |
| **Date Generated:** | 07/22/2020 | **Sections:** | 2 |
| **Date Revised:** |  | **Amendments:** | 0 |
| **Call Order:** | 007 | **Highway Number:** |  |
| **Items:** | 61 | **Counties:** | Cibola |
| **Project ID:** | 6100841 |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Proposal items table | | | | | |
| **Line** | **Item** | **Quantity** | **Unit** | **Description** | **Price** |
| **Section 0001: BRIDGE** | | | | | |
| 0010 | 210002 | 660.000 | C.Y. | MAJOR STRUCTURE EXCAVATION |  |
| 0020 | 210003 | 460.000 | C.Y. | MAJOR STRUCTURE BACKFILL |  |
| 0030 | 411000 | 86.000 | LB | HOT POURED CRACK SEALING |  |
| 0040 | 511000 | 19.000 | C.Y. | STRUCTURAL CONCRETE, CLASS A |  |
| 0050 | 511070 | 245.000 | C.Y. | STRUCTURAL CONCRETE, CLASS HPD |  |
| 0060 | 515000 | 18.000 | C.Y. | REINF.CONCRETE FOR MINOR STRUCTURES |  |
| 0070 | 529000 | 1.000 | LS | PIER AND ABUTMENT BEARING MODIFICATIONS |  |
| 0080 | 533000 | 138.000 | S.Y. | REPAIR OF CONCRETE STRUCTURES |  |
| 0090 | 533001 | 90.000 | EACH | EMBEDDED GALVANIC ANODES |  |
| 0100 | 533003 | 200.000 | LB | REPLACEMENT REINFORCING BARS |  |
| 0110 | 534000 | 10.000 | GAL | EPOXY INJECTION, TYPE I |  |
| 0120 | 535100 | 2,699.000 | S.Y. | CONCRETE SURFACE TREATMENT |  |
| 0130 | 536001 | 2,699.000 | S.Y. | EPOXY URETHANE POLYMER CONCRETE BRIDGE DECK OVERLAY |  |
| 0140 | 540060 | 890.000 | LB | REINFORCING BARS GRADE 60 |  |
| 0150 | 540160 | 35,540.000 | LB | EPOXY COATED REINFORCING BARS GRADE 60 |  |
| 0160 | 541100 | 8,369.000 | LB | STRUCTURAL STEEL FOR STEEL BRIDGES |  |
| 0170 | 541101 | 1.000 | LS | HEAT STRAIGHTENING STEEL STRUCTURES |  |
| 0180 | 543002 | 614.000 | L.F. | METAL RAILING, TYPE A42 |  |
| 0190 | 546000 | 1.000 | LS | RECOATING STRUCTURES |  |
| 0200 | 546200 | 3,053.000 | S.F. | SP 3 POWER TOOL CLEANING |  |
| 0210 | 546210 | 95.000 | S.F. | SP 11 POWER TOOL CLEANING |  |
| 0220 | 560000 | 24.000 | EACH | ELASTOMERIC BEARING PADS |  |
| 0230 | 562000 | 160.000 | L.F. | BRIDGE JOINT STRIP SEAL |  |
| 0240 | 601000 | 1.000 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  |
| 0250 | 602000 | 7.000 | C.Y. | RIPRAP CLASS A |  |
| 0260 | 602060 | 50.000 | S.Y. | RIPRAP CLASS G |  |
| 0270 | 604300 | 1,970.000 | S.Y. | GEOGRID REINFORCEMENT |  |
| **Section 0002: ROADWAY** | | | | | |
| 0280 | 203000 | 1,250.000 | C.Y. | UNCLASSIFIED EXCAVATION |  |
| 0290 | 207000 | 230.000 | S.Y. | SUBGRADE PREPARATION |  |
| 0300 | 303000 | 70.000 | TON | BASE COURSE |  |
| 0310 | 405000 | 4,100.000 | S.Y. | DETOUR PAVEMENT CONSTRUCTION |  |
| 0320 | 414000 | 200.000 | SYIN | COLD MILLING (ASPHALT) |  |
| 0330 | 416013 | 350.000 | TON | MINOR PAVEMENT HMA SP-III |  |
| 0340 | 547000 | 1.000 | LS | SAFETY AND ENVIRONMENTAL REQUIREMENTS |  |
| 0350 | 603281 | 1.000 | LS | SWPPP PLAN PREPARATION AND MAINTENANCE |  |
| 0360 | 604310 | 7,950.000 | S.Y. | GEOGRID BASE REINFORCEMENT |  |
| 0370 | 606001 | 150.000 | L.F. | SINGLE FACE W-BEAM GUARDRAIL |  |
| 0380 | 606051 | 1.000 | EACH | END TREATMENT TL-3 END TERMINAL |  |
| 0390 | 606053 | 3.000 | EACH | END TREATMENT W-BEAM END ANCHOR |  |
| 0400 | 606062 | 4.000 | EACH | TRANSITION METAL BARRIER TO RIGID BARRIER |  |
| 0410 | 606598 | 380.000 | L.F. | TCWB RETAINED BY THE CONTRACTOR |  |
| 0420 | 618000 | 1.000 | LS | TRAFFIC CONTROL MANAGEMENT |  |
| 0430 | 618011 | 1.000 | LS | PUBLIC AWARENESS | $15,000.00000 |
| 0440 | 621000 | 1.000 | LS | MOBILIZATION |  |
| 0450 | 632000 | 1.000 | ACRE | CLASS A SEEDING |  |
| 0460 | 632020 | 0.100 | ACRE | CLASS C SEEDING |  |
| 0470 | 702000 | 294.000 | S.F. | CONSTRUCTION SIGNING |  |
| 0480 | 702100 | 352.000 | L.F. | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING |  |
| 0490 | 702101 | 15.000 | EACH | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING |  |
| 0500 | 702610 | 5.000 | EACH | PORTABLE CHANGEABLE MESSAGE SIGN |  |
| 0510 | 702810 | 1.000 | LS | TRAFFIC CONTROL DEVICES FOR CONSTRUCTION |  |
| 0520 | 704000 | 7,000.000 | L.F. | RETROREFLECTORIZED PAINTED MARKINGS 4" |  |
| 0530 | 704002 | 7,250.000 | L.F. | RETROREFLECTORIZED PAINTED MARKINGS 6" |  |
| 0540 | 704005 | 50.000 | L.F. | RETROREFLECTORIZED PAINTED MARKINGS 24" |  |
| 0550 | 704099 | 19,686.000 | L.F. | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" |  |
| 0560 | 720060 | 1.000 | EACH | VEHICULAR IMPACT ATTENUATOR UNIT-WORK ZONES |  |
| 0570 | 721000 | 8,288.000 | L.F. | REMOVAL OF PAVEMENT MARKING |  |
| 0580 | 801000 | 1.000 | LS | CONSTRUCTION STAKING BY THE CONTRACTOR |  |
| 0590 | 802000 | 1.000 | LS | POST CONSTRUCTION PLANS | $40,100.00000 |
| 0600 | 803000 | 1.000 | LS | SCHEDULE SOFTWARE |  |
| 0610 | 803020 | 1.000 | LS | CPM HARDWARE/EQUIPMENT |  |

|  |  |  |
| --- | --- | --- |
|  | **Proposal 6101206R** |  |

Driveway Turnout Construction, Guardrail Installation

|  |  |  |  |
| --- | --- | --- | --- |
| Proposal information table | | | |
| **Date Generated:** | 07/22/2020 | **Sections:** | 1 |
| **Date Revised:** |  | **Amendments:** | 0 |
| **Call Order:** | 008 | **Highway Number:** |  |
| **Items:** | 34 | **Counties:** | Catron |
| **Project ID:** | 6101206R |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Proposal items table | | | | | |
| **Line** | **Item** | **Quantity** | **Unit** | **Description** | **Price** |
| **Section 0001: ROADWAY** | | | | | |
| 0010 | 201000 | 1.000 | LS | CLEARING AND GRUBBING |  |
| 0020 | 203000 | 63.000 | C.Y. | UNCLASSIFIED EXCAVATION |  |
| 0030 | 203100 | 295.000 | C.Y. | BORROW |  |
| 0040 | 207000 | 410.000 | S.Y. | SUBGRADE PREPARATION |  |
| 0050 | 303000 | 130.000 | TON | BASE COURSE |  |
| 0060 | 408100 | 0.300 | TON | PRIME COAT MATERIAL |  |
| 0070 | 417000 | 150.000 | S.Y. | MISCELLANEOUS PAVING |  |
| 0080 | 570437 | 58.000 | L.F. | 24" STORM DRAIN CULVERT PIPE |  |
| 0090 | 601000 | 1.000 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  |
| 0100 | 601110 | 60.000 | S.Y. | REMOVAL OF SURFACING |  |
| 0110 | 602010 | 30.000 | C.Y. | RIPRAP CLASS B |  |
| 0120 | 602060 | 44.000 | S.Y. | RIPRAP CLASS G |  |
| 0130 | 603100 | 0.100 | ACRE | TEMPORARY SOIL STABILANT |  |
| 0140 | 603250 | 1.000 | EACH | DROP INLET PROTECTION TYPE I |  |
| 0150 | 604310 | 350.000 | S.Y. | GEOGRID BASE REINFORCEMENT |  |
| 0160 | 606001 | 62.500 | L.F. | SINGLE FACE W-BEAM GUARDRAIL |  |
| 0170 | 606055 | 1.000 | EACH | END TREATMENT DRIVEWAY END ANCHOR |  |
| 0180 | 606063 | 1.000 | EACH | EXISTING BEAM GUARDRAIL TO 31" BEAM GUARDRAIL TRANSITION |  |
| 0190 | 607004 | 75.000 | L.F. | BARBED WIRE FENCE 4' |  |
| 0200 | 607015 | 4.000 | EACH | BRACES/CORNER POSTS |  |
| 0210 | 607314 | 1.000 | EACH | STANDARD GATE, 14' |  |
| 0220 | 617000 | 1.000 | LS | VIBRATION MONITORING |  |
| 0230 | 617003 | 1.000 | LS | VIDEO RECORDING |  |
| 0240 | 617004 | 1.000 | LS | VIBRATION RISK SURVEY |  |
| 0250 | 618000 | 1.000 | LS | TRAFFIC CONTROL MANAGEMENT |  |
| 0260 | 621000 | 1.000 | LS | MOBILIZATION |  |
| 0270 | 623000 | 1.000 | EACH | MEDIAN DROP INLET TYPE I (URBAN) H=0'0" TO 3'0" |  |
| 0280 | 632000 | 0.100 | ACRE | CLASS A SEEDING |  |
| 0290 | 662450 | 1.000 | EACH | TIE TO EXISTING MANHOLE |  |
| 0300 | 702810 | 1.000 | LS | TRAFFIC CONTROL DEVICES FOR CONSTRUCTION |  |
| 0310 | 801000 | 1.000 | LS | CONSTRUCTION STAKING BY THE CONTRACTOR |  |
| 0320 | 802000 | 1.000 | LS | POST CONSTRUCTION PLANS | $1,000.00000 |
| 0330 | 803000 | 1.000 | LS | SCHEDULE SOFTWARE |  |
| 0340 | 803020 | 1.000 | LS | CPM HARDWARE/EQUIPMENT |  |