Date Generated

**Dec 18, 2022**

Call Order

**001**

Project ID

**A302123**

Amendments

**0**

Counties

**Bernalillo**

Highway Number

Time Remaining

Add to calendar

Days

**17**

Hours

**21**

Description

**Roadway Rehabilitation and Reconstruction**

Edit favorites

Export

| **Line** | **Item** | **Description** | **Unit** | **Quantity** | **Price** | |
| --- | --- | --- | --- | --- | --- | --- |
| Section 0001: ROADWAY | | | | | | |
| 0010 | 201000 | CLEARING AND GRUBBING | LS | 1 |  |  |
| 0020 | 203000 | UNCLASSIFIED EXCAVATION | C.Y. | 290 |  |  |
| 0030 | 203211 | UNSTABLE SUBGRADE STABILIZATION | S.Y. | 290 |  |  |
| 0040 | 203301 | ROCK EXCAVATION | C.Y. | 90 |  |  |
| 0050 | 207000 | SUBGRADE PREPARATION | S.Y. | 630 |  |  |
| 0060 | 303000 | BASE COURSE | TON | 320 |  |  |
| 0070 | 403705 | WARM MIX OPEN-GRADED FRICTION COURSE COMPLETE | TON | 7900 |  |  |
| 0080 | 405000 | DETOUR PAVEMENT CONSTRUCTION | S.Y. | 8700 |  |  |
| 0090 | 407000 | ASPHALT MATERIAL FOR TACK COAT | TON | 273 |  |  |
| 0100 | 407001 | FOG SEAL | TON | 130 |  |  |
| 0110 | 408100 | PRIME COAT MATERIAL | TON | 3 |  |  |
| 0120 | 414000 | COLD MILLING (ASPHALT) | SYIN | 1456900 |  |  |
| 0130 | 416217 | MINOR PAVING TYPE II, WMA SP-IV | S.Y. | 280 |  |  |
| 0140 | 424004 | WMA SP-IV COMPLETE | TON | 75560 |  |  |
| 0150 | 570037 | 36" CULVERT PIPE END SECTION | EACH | 1 |  |  |
| 0160 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| 0170 | 601110 | REMOVAL OF SURFACING | S.Y. | 910 |  |  |
| 0180 | 602010 | RIPRAP CLASS B | C.Y. | 80 |  |  |
| 0190 | 602020 | RIPRAP CLASS C | C.Y. | 110 |  |  |
| 0200 | 603100 | TEMPORARY SOIL STABILANT | ACRE | 1.2 |  |  |
| 0210 | 606001 | SINGLE FACE W-BEAM GUARDRAIL | L.F. | 2700 |  |  |
| 0220 | 606051 | END TREATMENT TL-3 END TERMINAL | EACH | 3 |  |  |
| 0230 | 607012 | GAME FENCE | L.F. | 590 |  |  |
| 0240 | 607015 | BRACES/CORNER POSTS | EACH | 44 |  |  |
| 0250 | 609324 | CONCRETE SLOPED CURB AND GUTTER 6" X 24" | L.F. | 620 |  |  |
| 0260 | 609330 | CONCRETE SLOPED CURB AND GUTTER 6" X 30" | L.F. | 1620 |  |  |
| 0270 | 610080 | GAME GUARD | L.F. | 210 |  |  |
| 0280 | 618000 | TRAFFIC CONTROL MANAGEMENT | LS | 1 |  |  |
| 0290 | 618011 | PUBLIC AWARENESS | LS | 1 | $10,000.00 |  |
| 0300 | 621000 | MOBILIZATION | LS | 1 |  |  |
| 0310 | 631000 | RUMBLE STRIPS | L.F. | 115600 |  |  |
| 0320 | 632000 | CLASS A SEEDING | ACRE | 1 |  |  |
| 0330 | 663049 | PRECONSTRUCTION UTILITY SURVEY | LS | 1 |  |  |
| 0340 | 701000 | PANEL SIGNS | S.F. | 1784 |  |  |
| 0350 | 701100 | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS | L.F. | 2982 |  |  |
| 0360 | 701101 | MULTI-DIRECTIONAL SLIP BASE POSTS FOR ALUMINUM PANEL SIGNS | EACH | 6 |  |  |
| 0370 | 702000 | CONSTRUCTION SIGNING | S.F. | 196 |  |  |
| 0380 | 702100 | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING | L.F. | 217 |  |  |
| 0390 | 702101 | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING | EACH | 12 |  |  |
| 0400 | 702610 | PORTABLE CHANGEABLE MESSAGE SIGN | EACH | 17 |  |  |
| 0410 | 702810 | TRAFFIC CONTROL DEVICES FOR CONSTRUCTION | LS | 1 |  |  |
| 0420 | 702850 | LAW ENFORCEMENT IN CONSTRUCTION ZONE | ALOW | 1 | $15,000.00 |  |
| 0430 | 703100 | ROAD DELINEATOR TYPE GUIDE | EACH | 48 |  |  |
| 0440 | 703300 | REFLECTIVE BARRIER DELINEATOR | EACH | 397 |  |  |
| 0450 | 703400 | 1/10TH MILE DELINEATOR | EACH | 108 |  |  |
| 0460 | 704000 | RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 900 |  |  |
| 0470 | 704002 | RETROREFLECTORIZED PAINTED MARKINGS 6" | L.F. | 432100 |  |  |
| 0480 | 704004 | RETROREFLECTORIZED PAINTED MARKINGS 12" | L.F. | 2500 |  |  |
| 0490 | 704027 | RETROREFLECTORIZED PAINTED MARKING RIGHT LANE DROP ARROW | EACH | 6 |  |  |
| 0500 | 704099 | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 337317 |  |  |
| 0510 | 704700 | HOT THERMOPLASTIC PAVEMENT MARKINGS 4" | L.F. | 61200 |  |  |
| 0520 | 704701 | HOT THERMOPLASTIC PAVEMENT MARKINGS 6" | L.F. | 12100 |  |  |
| 0530 | 704702 | HOT THERMOPLASTIC PAVEMENT MARKINGS 8" | L.F. | 3000 |  |  |
| 0540 | 704704 | HOT THERMOPLASTIC PAVEMENT MARKING 24" | L.F. | 200 |  |  |
| 0550 | 704706 | HOT THERMOPLASTIC PAVEMENT MARKINGS 12" | L.F. | 26300 |  |  |
| 0560 | 704717 | HOT THERMOPLASTIC PAVEMENT MARKING RIGHT ARROW | EACH | 3 |  |  |
| 0570 | 704718 | HOT THERMOPLASTIC PAVEMENT MARKING LEFT ARROW | EACH | 3 |  |  |
| 0580 | 704720 | HOT THERMOPLASTIC PAVEMENT MARKING WORD (ONLY) | EACH | 4 |  |  |
| 0590 | 704739 | HOT THERMOPLASTIC PAVEMENT MARKING WRONG WAY ARROW | EACH | 11 |  |  |
| 0600 | 704869 | PLOWABLE REFLECTIVE RAISED PAVEMENT MARKER TYPE PG | EACH | 258 |  |  |
| 0610 | 704871 | PLOWABLE REFLECTIVE RAISED PAVEMENT MARKER TYPE PJ | EACH | 24 |  |  |
| 0620 | 704872 | PLOWABLE REFLECTIVE RAISED PAVEMENT MARKER TYPE PC | EACH | 189 |  |  |
| 0630 | 704876 | TEMPORARY REFLECTIVE RAISED PAVEMENT MARKER, TYPE TG | EACH | 7118 |  |  |
| 0640 | 704877 | TEMPORARY REFLECTIVE RAISED PAVEMENT MARKER, TYPE TH | EACH | 1504 |  |  |
| 0650 | 801000 | CONSTRUCTION STAKING BY THE CONTRACTOR | LS | 1 |  |  |
| 0660 | 802000 | POST CONSTRUCTION PLANS | LS | 1 | $6,000.00 |  |

Date Generated

**Dec 18, 2022**

Call Order

**002**

Project ID

**1101920**

Amendments

**0**

Counties

**Socorro**

Highway Number

Time Remaining

Add to calendar

Days

**17**

Hours

**21**

Description

**Roadway Rehabilitation**

Export

| **Line** | **Item** | **Description** | **Unit** | **Quantity** | **Price** | |
| --- | --- | --- | --- | --- | --- | --- |
| Section 0001: ROADWAY | | | | | | |
| 0010 | 403715 | RUBBERIZED OPEN-GRADED FRICTION COURSE COMPLETE | TON | 6340 |  |  |
| 0020 | 407000 | ASPHALT MATERIAL FOR TACK COAT | TON | 229 |  |  |
| 0030 | 414000 | COLD MILLING (ASPHALT) | SYIN | 1414000 |  |  |
| 0040 | 423283 | HMA SP-IV COMPLETE | TON | 67846 |  |  |
| 0050 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| 0060 | 606001 | SINGLE FACE W-BEAM GUARDRAIL | L.F. | 16900 |  |  |
| 0070 | 606051 | END TREATMENT TL-3 END TERMINAL | EACH | 39 |  |  |
| 0080 | 606053 | END TREATMENT W-BEAM END ANCHOR | EACH | 20 |  |  |
| 0090 | 606062 | TRANSITION METAL BARRIER TO RIGID BARRIER | EACH | 48 |  |  |
| 0100 | 606542 | CONCRETE WALL BARRIER 42" | L.F. | 2058 |  |  |
| 0110 | 606554 | CONCRETE WALL BARRIER 54" | L.F. | 436 |  |  |
| 0120 | 618000 | TRAFFIC CONTROL MANAGEMENT | LS | 1 |  |  |
| 0130 | 621000 | MOBILIZATION | LS | 1 |  |  |
| 0140 | 630100 | MULTIPLE GLARE SHIELDING 24 IN | L.F. | 17382 |  |  |
| 0150 | 631000 | RUMBLE STRIPS | L.F. | 115640 |  |  |
| 0160 | 701000 | PANEL SIGNS | S.F. | 892 |  |  |
| 0170 | 701100 | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS | L.F. | 2295 |  |  |
| 0180 | 702000 | CONSTRUCTION SIGNING | S.F. | 1600 |  |  |
| 0190 | 702100 | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING | L.F. | 948 |  |  |
| 0200 | 702101 | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING | EACH | 12 |  |  |
| 0210 | 702110 | PORTABLE SIGN SUPPORT | EACH | 62 |  |  |
| 0220 | 702238 | BARRICADE, TYPE III-8' | EACH | 2 |  |  |
| 0230 | 702525 | CHANNELIZATION DEVICES TYPE DRUM | EACH | 480 |  |  |
| 0240 | 702600 | SEQUENTIAL ARROW DISPLAY | EACH | 2 |  |  |
| 0250 | 702610 | PORTABLE CHANGEABLE MESSAGE SIGN | EACH | 8 |  |  |
| 0260 | 703100 | ROAD DELINEATOR TYPE GUIDE | EACH | 30 |  |  |
| 0270 | 704099 | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 158600 |  |  |
| 0280 | 704700 | HOT THERMOPLASTIC PAVEMENT MARKINGS 4" | L.F. | 20200 |  |  |
| 0290 | 704701 | HOT THERMOPLASTIC PAVEMENT MARKINGS 6" | L.F. | 156000 |  |  |
| 0300 | 704704 | HOT THERMOPLASTIC PAVEMENT MARKING 24" | L.F. | 40 |  |  |
| 0310 | 704706 | HOT THERMOPLASTIC PAVEMENT MARKINGS 12" | L.F. | 7300 |  |  |
| 0320 | 704739 | HOT THERMOPLASTIC PAVEMENT MARKING WRONG WAY ARROW | EACH | 8 |  |  |
| 0330 | 704869 | PLOWABLE REFLECTIVE RAISED PAVEMENT MARKER TYPE PG | EACH | 120 |  |  |
| 0340 | 704871 | PLOWABLE REFLECTIVE RAISED PAVEMENT MARKER TYPE PJ | EACH | 3540 |  |  |
| 0350 | 704872 | PLOWABLE REFLECTIVE RAISED PAVEMENT MARKER TYPE PC | EACH | 1870 |  |  |
| 0360 | 720050 | PERMANENT VEHICULAR IMPACT ATTENUATOR UNIT | EACH | 1 |  |  |
| 0370 | 721000 | REMOVAL OF PAVEMENT MARKING | L.F. | 970 |  |  |
| 0380 | 801000 | CONSTRUCTION STAKING BY THE CONTRACTOR | LS | 1 |  |  |
| 0390 | 802000 | POST CONSTRUCTION PLANS | LS | 1 | $5,000.00 |  |

Date Generated

**Dec 18, 2022**

Call Order

**003**

Project ID

**2104510**

Amendments

**0**

Counties

**De Baca**

Highway Number

Time Remaining

Add to calendar

Days

**17**

Hours

**21**

Description

**Bridge Rehabilitation, Roadway Rehabilitation/Reconstruction**

Edit favorites

Export

| **Line** | **Item** | **Description** | **Unit** | **Quantity** | **Price** | |
| --- | --- | --- | --- | --- | --- | --- |
| Section 0001: BRIDGE | | | | | | |
| 0010 | 210001 | UNSUITABLE MATERIAL EXCAVATION | C.Y. | 350 |  |  |
| 0020 | 210002 | MAJOR STRUCTURE EXCAVATION | C.Y. | 880 |  |  |
| 0030 | 210003 | MAJOR STRUCTURE BACKFILL | C.Y. | 510 |  |  |
| 0040 | 411000 | HOT POURED CRACK SEALING | LB | 300 |  |  |
| 0050 | 455000 | DIAMOND GRINDING OF PCCP | S.Y. | 320 |  |  |
| 0060 | 511070 | STRUCTURAL CONCRETE, CLASS HPD | C.Y. | 406 |  |  |
| 0070 | 533000 | REPAIR OF CONCRETE STRUCTURES | S.Y. | 48 |  |  |
| 0080 | 534000 | EPOXY INJECTION, TYPE I | GAL | 6 |  |  |
| 0090 | 535000 | CRACK SEALING | L.F. | 306 |  |  |
| 0100 | 536001 | EPOXY URETHANE POLYMER CONCRETE BRIDGE DECK OVERLAY | S.Y. | 1388 |  |  |
| 0110 | 540061 | GALVANIZED BARS GRADE 60 | LB | 107500 |  |  |
| 0120 | 543002 | METAL RAILING, TYPE A42 | L.F. | 466 |  |  |
| 0130 | 546000 | RECOATING STRUCTURES | LS | 1 |  |  |
| 0140 | 546200 | SP 3 POWER TOOL CLEANING | S.F. | 100 |  |  |
| 0150 | 546210 | SP 11 POWER TOOL CLEANING | S.F. | 1100 |  |  |
| 0160 | 562000 | BRIDGE JOINT STRIP SEAL | L.F. | 122 |  |  |
| 0170 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| 0180 | 604002 | GEOTEXTILE CLASS 2 | S.Y. | 1760 |  |  |
| 0190 | 604300 | GEOGRID REINFORCEMENT | S.Y. | 1520 |  |  |
| Section 0002: ROADWAY | | | | | | |
| 0200 | 403701 | OPEN GRADED FRICTION COURSE COMPLETE | TON | 80 |  |  |
| 0210 | 407000 | ASPHALT MATERIAL FOR TACK COAT | TON | 3 |  |  |
| 0220 | 408100 | PRIME COAT MATERIAL | TON | 1 |  |  |
| 0230 | 414000 | COLD MILLING (ASPHALT) | SYIN | 14200 |  |  |
| 0240 | 416104 | MINOR PAVING TYPE I, HMA SP-IV | TON | 920 |  |  |
| 0250 | 547000 | SAFETY AND ENVIRONMENTAL REQUIREMENTS | LS | 1 |  |  |
| 0260 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| 0270 | 606001 | SINGLE FACE W-BEAM GUARDRAIL | L.F. | 387.5 |  |  |
| 0280 | 606051 | END TREATMENT TL-3 END TERMINAL | EACH | 4 |  |  |
| 0290 | 606062 | TRANSITION METAL BARRIER TO RIGID BARRIER | EACH | 4 |  |  |
| 0300 | 606710 | TCWB RETAINED BY THE CONTRACTOR (20') | L.F. | 880 |  |  |
| 0310 | 606719 | RESETTING OF TCWB (20') | L.F. | 1760 |  |  |
| 0320 | 618000 | TRAFFIC CONTROL MANAGEMENT | LS | 1 |  |  |
| 0330 | 621000 | MOBILIZATION | LS | 1 |  |  |
| 0340 | 702000 | CONSTRUCTION SIGNING | S.F. | 784 |  |  |
| 0350 | 702100 | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING | L.F. | 1946 |  |  |
| 0360 | 702101 | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING | EACH | 6 |  |  |
| 0370 | 702110 | PORTABLE SIGN SUPPORT | EACH | 20 |  |  |
| 0380 | 702238 | BARRICADE, TYPE III-8' | EACH | 2 |  |  |
| 0390 | 702525 | CHANNELIZATION DEVICES TYPE DRUM | EACH | 72 |  |  |
| 0400 | 702610 | PORTABLE CHANGEABLE MESSAGE SIGN | EACH | 2 |  |  |
| 0410 | 702613 | SPEED DETECTOR RADAR TRAILER | EACH | 2 |  |  |
| 0420 | 704000 | RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 11400 |  |  |
| 0430 | 704100 | REMOVABLE MARKING TAPE 4" | L.F. | 5185 |  |  |
| 0440 | 720060 | VEHICULAR IMPACT ATTENUATOR UNIT-WORK ZONES | EACH | 4 |  |  |
| 0450 | 720110 | REMOVE/RESET IMPACT ATTENUATOR UNIT | EACH | 8 |  |  |
| 0460 | 721000 | REMOVAL OF PAVEMENT MARKING | L.F. | 800 |  |  |
| 0470 | 801000 | CONSTRUCTION STAKING BY THE CONTRACTOR | LS | 1 |  |  |
| 0480 | 802000 | POST CONSTRUCTION PLANS | LS | 1 | $7,500.00 |  |
| 0490 | 803000 | SCHEDULE SOFTWARE | LS | 1 |  |  |
| 0500 | 803020 | CPM HARDWARE/EQUIPMENT | LS | 1 |  |  |

Date Generated

**Dec 18, 2022**

Call Order

**004**

Project ID

**1102110**

Amendments

**0**

Counties

**Dona Ana Grant Hidalgo Luna**

Highway Number

Time Remaining

Add to calendar

Days

**17**

Hours

**21**

Description

**ITS (Truck Availability Parking System and CCTV Cameras)**

Edit favorites

Export

| **Line** | **Item** | **Description** | **Unit** | **Quantity** | **Price** | |
| --- | --- | --- | --- | --- | --- | --- |
| Section 0001: ROADWAY | | | | | | |
| 0010 | 201000 | CLEARING AND GRUBBING | LS | 1 |  |  |
| 0020 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| 0030 | 618000 | TRAFFIC CONTROL MANAGEMENT | LS | 1 |  |  |
| 0040 | 621000 | MOBILIZATION | LS | 1 |  |  |
| 0050 | 701109 | STEEL I-BEAM POST TYPE W6X9 | L.F. | 20 |  |  |
| 0060 | 701118 | STEEL I-BEAM POST TYPE W8X18 | L.F. | 30 |  |  |
| 0070 | 701121 | STEEL I-BEAM POST TYPE W8X21 | L.F. | 140 |  |  |
| 0080 | 701124 | STEEL I-BEAM POST TYPE W8X24 | L.F. | 30 |  |  |
| 0090 | 701209 | BREAKAWAY BASE SYSTEM FOR STEEL I BEAM POST W6X9 | EACH | 2 |  |  |
| 0100 | 701218 | BREAKAWAY BASE SYSTEM FOR STEEL I BEAM POST W8X18 | EACH | 2 |  |  |
| 0110 | 701221 | BREAKAWAY BASE SYSTEM FOR STEEL I BEAM POST W8X21 | EACH | 10 |  |  |
| 0120 | 701224 | BREAKAWAY BASE SYSTEM FOR STEEL I BEAM POST W8X24 | EACH | 2 |  |  |
| 0130 | 702000 | CONSTRUCTION SIGNING | S.F. | 1140 |  |  |
| 0140 | 702100 | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING | L.F. | 530 |  |  |
| 0150 | 702101 | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING | EACH | 12 |  |  |
| 0160 | 702110 | PORTABLE SIGN SUPPORT | EACH | 40 |  |  |
| 0170 | 702238 | BARRICADE, TYPE III-8' | EACH | 2 |  |  |
| 0180 | 702525 | CHANNELIZATION DEVICES TYPE DRUM | EACH | 154 |  |  |
| 0190 | 702600 | SEQUENTIAL ARROW DISPLAY | EACH | 2 |  |  |
| 0200 | 702610 | PORTABLE CHANGEABLE MESSAGE SIGN | EACH | 2 |  |  |
| 0210 | 706200 | METER PEDESTAL (SIGNAL) | EACH | 2 |  |  |
| 0220 | 706350 | POWER SERVICE INSTALLATION | LS | 1 | $35,000.00 |  |
| 0230 | 711102 | SINGLE CONDUCTOR 2 | L.F. | 31410 |  |  |
| 0240 | 750000 | INTELLIGENT TRANSPORTATION SYSTEM | LS | 1 |  |  |
| 0250 | 750024 | COMMUNICATIONS CONDUIT 4" | L.F. | 7490 |  |  |
| 0260 | 750032 | MULTI-DUCT CONDUIT 2" (8-WAY) | L.F. | 30510 |  |  |
| 0270 | 750060 | ITS PULLBOX (33"X24"X24") | EACH | 64 |  |  |
| 0280 | 750080 | ITS MANHOLE (48"X48"X48") | EACH | 4 |  |  |
| 0290 | 750100 | CLOSED CIRCUIT TELEVISION SYSTEM (CCTV) | EACH | 5 |  |  |
| 0300 | 750110 | CAMERA LOWERING DEVICE | EACH | 5 |  |  |
| 0310 | 750230 | ITS CONCRETE POLE, 30 FT | EACH | 7 |  |  |
| 0320 | 750250 | ITS CONCRETE POLE, 50 FT | EACH | 5 |  |  |

Date Generated

**Dec 21, 2022**

Call Order

**005**

Project ID

**5100470**

Amendments

**0**

Counties

**Socorro**

Highway Number

Time Remaining

Add to calendar

Days

**17**

Hours

**21**

Description

**Bridge Replacement, Roadway Reconstruction**

Edit favorites

Export

| **Line** | **Item** | **Description** | **Unit** | **Quantity** | **Price** | |
| --- | --- | --- | --- | --- | --- | --- |
| Section 0001: BRIDGE | | | | | | |
| 0010 | 210002 | MAJOR STRUCTURE EXCAVATION | C.Y. | 835 |  |  |
| 0020 | 210003 | MAJOR STRUCTURE BACKFILL | C.Y. | 760 |  |  |
| 0030 | 502042 | DRILLED SHAFT FOUNDATION 42" DIAMETER | L.F. | 255 |  |  |
| 0040 | 502048 | DRILLED SHAFT FOUNDATION 48" DIAMETER | L.F. | 135 |  |  |
| 0050 | 502154 | PERMANENT CASING 54" DIAMETER | L.F. | 66 |  |  |
| 0060 | 502600 | OBSTRUCTION REMOVAL | L.F. | 75 |  |  |
| 0070 | 505001 | CROSSHOLE SONIC LOGGING DEPARTMENT TESTING | EACH | 9 |  |  |
| 0080 | 505010 | LOW STRAIN INTEGRITY DEPARTMENT TESTING | EACH | 9 |  |  |
| 0090 | 511000 | STRUCTURAL CONCRETE, CLASS A | C.Y. | 130 |  |  |
| 0100 | 511070 | STRUCTURAL CONCRETE, CLASS HPD | C.Y. | 520 |  |  |
| 0110 | 514042 | CONCRETE BARRIER RAILINGS 42" | L.F. | 424 |  |  |
| 0120 | 515000 | REINF.CONCRETE FOR MINOR STRUCTURES | C.Y. | 20 |  |  |
| 0130 | 518045 | PRESTRESSED CONCRETE BRIDGE MEMBER TYPE 45 | L.F. | 847 |  |  |
| 0140 | 535100 | CONCRETE SURFACE TREATMENT | S.Y. | 1175 |  |  |
| 0150 | 536001 | EPOXY URETHANE POLYMER CONCRETE BRIDGE DECK OVERLAY | S.Y. | 1175 |  |  |
| 0160 | 540060 | REINFORCING BARS GRADE 60 | LB | 54760 |  |  |
| 0170 | 540061 | GALVANIZED BARS GRADE 60 | LB | 97000 |  |  |
| 0180 | 541000 | STRUCTURAL STEEL FOR CONCRETE BRIDGES | LB | 6075 |  |  |
| 0190 | 560000 | ELASTOMERIC BEARING PADS | EACH | 20 |  |  |
| 0200 | 562000 | BRIDGE JOINT STRIP SEAL | L.F. | 109 |  |  |
| 0210 | 565000 | PREFORMED SILICONE-COATED FOAM JOINT SYSTEM | L.F. | 104 |  |  |
| 0220 | 570036 | 36" CULVERT PIPE | L.F. | 32 |  |  |
| 0230 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| 0240 | 602000 | RIPRAP CLASS A | C.Y. | 10 |  |  |
| 0250 | 602060 | RIPRAP CLASS G | S.Y. | 14 |  |  |
| 0260 | 604300 | GEOGRID REINFORCEMENT | S.Y. | 2480 |  |  |
| Section 0002: ROADWAY | | | | | | |
| 0270 | 201000 | CLEARING AND GRUBBING | LS | 1 |  |  |
| 0280 | 203000 | UNCLASSIFIED EXCAVATION | C.Y. | 50 |  |  |
| 0290 | 203100 | BORROW | C.Y. | 4575 |  |  |
| 0300 | 203301 | ROCK EXCAVATION | C.Y. | 7325 |  |  |
| 0310 | 207000 | SUBGRADE PREPARATION | S.Y. | 3710 |  |  |
| 0320 | 303000 | BASE COURSE | TON | 1145 |  |  |
| 0330 | 403701 | OPEN GRADED FRICTION COURSE COMPLETE | TON | 75 |  |  |
| 0340 | 405000 | DETOUR PAVEMENT CONSTRUCTION | S.Y. | 7310 |  |  |
| 0350 | 407000 | ASPHALT MATERIAL FOR TACK COAT | TON | 3 |  |  |
| 0360 | 408100 | PRIME COAT MATERIAL | TON | 7 |  |  |
| 0370 | 423282 | HMA SP-III COMPLETE | TON | 1285 |  |  |
| 0380 | 570048 | 48" CULVERT PIPE | L.F. | 180 |  |  |
| 0390 | 570072 | 72" CULVERT PIPE | L.F. | 320 |  |  |
| 0400 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| 0410 | 601110 | REMOVAL OF SURFACING | S.Y. | 3485 |  |  |
| 0420 | 602010 | RIPRAP CLASS B | C.Y. | 85 |  |  |
| 0430 | 602020 | RIPRAP CLASS C | C.Y. | 2470 |  |  |
| 0440 | 603281 | SWPPP PLAN PREPARATION AND MAINTENANCE | LS | 1 |  |  |
| 0450 | 604001 | GEOTEXTILE CLASS 1 | S.Y. | 2345 |  |  |
| 0460 | 606001 | SINGLE FACE W-BEAM GUARDRAIL | L.F. | 437.5 |  |  |
| 0470 | 606051 | END TREATMENT TL-3 END TERMINAL | EACH | 4 |  |  |
| 0480 | 606061 | DRAINAGE STRUCTURE PROTECTION SYSTEM | L.F. | 200 |  |  |
| 0490 | 606062 | TRANSITION METAL BARRIER TO RIGID BARRIER | EACH | 4 |  |  |
| 0500 | 606598 | TCWB RETAINED BY THE CONTRACTOR | L.F. | 4220 |  |  |
| 0510 | 607004 | BARBED WIRE FENCE 4' | L.F. | 970 |  |  |
| 0520 | 607015 | BRACES/CORNER POSTS | EACH | 12 |  |  |
| 0530 | 618000 | TRAFFIC CONTROL MANAGEMENT | LS | 1 |  |  |
| 0540 | 618011 | PUBLIC AWARENESS | LS | 1 | $10,000.00 |  |
| 0550 | 621000 | MOBILIZATION | LS | 1 |  |  |
| 0560 | 622100 | SUPPLEMENTAL FIELD LABORATORY | EACH | 1 |  |  |
| 0570 | 701000 | PANEL SIGNS | S.F. | 12 |  |  |
| 0580 | 701100 | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS | L.F. | 15 |  |  |
| 0590 | 702000 | CONSTRUCTION SIGNING | S.F. | 98 |  |  |
| 0600 | 702100 | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING | L.F. | 96 |  |  |
| 0610 | 702101 | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING | EACH | 6 |  |  |
| 0620 | 702610 | PORTABLE CHANGEABLE MESSAGE SIGN | EACH | 2 |  |  |
| 0630 | 702810 | TRAFFIC CONTROL DEVICES FOR CONSTRUCTION | LS | 1 |  |  |
| 0640 | 704000 | RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 14200 |  |  |
| 0650 | 704099 | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 8010 |  |  |
| 0660 | 721000 | REMOVAL OF PAVEMENT MARKING | L.F. | 2510 |  |  |
| 0670 | 801000 | CONSTRUCTION STAKING BY THE CONTRACTOR | LS | 1 |  |  |
| 0680 | 802000 | POST CONSTRUCTION PLANS | LS | 1 | $15,000.00 |  |
| 0690 | 803000 | SCHEDULE SOFTWARE | LS | 1 |  |  |