Date Generated

**Mar 20, 2023**

Call Order

**001**

Project ID

**A302220**

Amendments

**0**

Counties

**Valencia**

Highway Number

Time Remaining

Add to calendar

Days

**24**

Hours

**3**

Description

**Bridge New Construction, Roadway Reconstruction**

Items

Favorite items only

Edit favorites

Export

| **Line** | **Item** | **Description** | **Unit** | **Quantity** | **Price** | |
| --- | --- | --- | --- | --- | --- | --- |
| Section 0001: BRIDGE | | | | | | |
| 0010 | 210001 | UNSUITABLE MATERIAL EXCAVATION | C.Y. | 4313 |  |  |
| 0020 | 210002 | MAJOR STRUCTURE EXCAVATION | C.Y. | 176 |  |  |
| 0030 | 210003 | MAJOR STRUCTURE BACKFILL | C.Y. | 5210 |  |  |
| 0040 | 501100 | PILE SPLICES | EACH | 222 |  |  |
| 0050 | 501101 | PILE CUT-OFFS | L.F. | 1772 |  |  |
| 0060 | 501116 | DRIVEN PILES (16" PIPE) | L.F. | 10217 |  |  |
| 0070 | 504310 | PILE DYNAMIC TEST DEPARTMENT TESTING | EACH | 8 |  |  |
| 0080 | 504315 | CASE PILE WAVE ANALYSIS TEST DEPARTMENT TESTING | EACH | 16 |  |  |
| 0090 | 506000 | MSE PANEL WALL | S.F. | 24208 |  |  |
| 0100 | 511030 | STRUCTURAL CONCRETE, CLASS AA | C.Y. | 1217 |  |  |
| 0110 | 511070 | STRUCTURAL CONCRETE, CLASS HPD | C.Y. | 554 |  |  |
| 0120 | 540060 | REINFORCING BARS GRADE 60 | LB | 205565 |  |  |
| 0130 | 540061 | GALVANIZED BARS GRADE 60 | LB | 121980 |  |  |
| 0140 | 541100 | STRUCTURAL STEEL FOR STEEL BRIDGES | LB | 462070 |  |  |
| 0150 | 543002 | METAL RAILING, TYPE A42 | L.F. | 754 |  |  |
| 0160 | 560000 | ELASTOMERIC BEARING PADS | EACH | 24 |  |  |
| 0170 | 562000 | BRIDGE JOINT STRIP SEAL | L.F. | 89 |  |  |
| 0180 | 563099 | POLYMER BRIDGE JOINT SEALS | L.F. | 85 |  |  |
| 0190 | 604300 | GEOGRID REINFORCEMENT | S.Y. | 9463 |  |  |
| 0200 | 607076 | PEDESTRIAN SCREENING FENCE, TYPE 1 | L.F. | 683 |  |  |
| Section 0002: ROADWAY | | | | | | |
| 0210 | 201000 | CLEARING AND GRUBBING | LS | 1 |  |  |
| 0220 | 203000 | UNCLASSIFIED EXCAVATION | C.Y. | 6000 |  |  |
| 0230 | 203100 | BORROW | C.Y. | 80100 |  |  |
| 0240 | 207000 | SUBGRADE PREPARATION | S.Y. | 30300 |  |  |
| 0250 | 303000 | BASE COURSE | TON | 8700 |  |  |
| 0260 | 407000 | ASPHALT MATERIAL FOR TACK COAT | TON | 8 |  |  |
| 0270 | 407001 | FOG SEAL | TON | 2 |  |  |
| 0280 | 408100 | PRIME COAT MATERIAL | TON | 44 |  |  |
| 0290 | 416114 | MINOR PAVING TYPE I, WMA SP-IV | TON | 5010 |  |  |
| 0300 | 416214 | MINOR PAVING TYPE II, WMA SP-IV | TON | 250 |  |  |
| 0310 | 570018 | 18" CULVERT PIPE | L.F. | 40 |  |  |
| 0320 | 570019 | 18" CULVERT PIPE END SECTION | EACH | 2 |  |  |
| 0330 | 570060 | 60" CULVERT PIPE | L.F. | 80 |  |  |
| 0340 | 570437 | 24" STORM DRAIN CULVERT PIPE | L.F. | 1360 |  |  |
| 0350 | 570441 | 24" STORM DRAIN CULVERT PIPE END SECTION | EACH | 5 |  |  |
| 0360 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| 0370 | 601110 | REMOVAL OF SURFACING | S.Y. | 7000 |  |  |
| 0380 | 601300 | DEMOLITION | LS | 1 |  |  |
| 0390 | 601995 | AC-ABATEMENT | L.F. | 835 |  |  |
| 0400 | 601996 | AC-ABATEMENT | S.F. | 8400 |  |  |
| 0410 | 602005 | RIPRAP CLASS A (NON-ENCLOSED) | C.Y. | 70 |  |  |
| 0420 | 602060 | RIPRAP CLASS G | S.Y. | 2700 |  |  |
| 0430 | 603100 | TEMPORARY SOIL STABILANT | ACRE | 14 |  |  |
| 0440 | 603262 | COMPOSTED MULCH SOCKS | L.F. | 3800 |  |  |
| 0450 | 603281 | SWPPP PLAN PREPARATION AND MAINTENANCE | LS | 1 |  |  |
| 0460 | 606001 | SINGLE FACE W-BEAM GUARDRAIL | L.F. | 1475 |  |  |
| 0470 | 606052 | END TREATMENT TL-2 END TERMINAL | EACH | 4 |  |  |
| 0480 | 606062 | TRANSITION METAL BARRIER TO RIGID BARRIER | EACH | 6 |  |  |
| 0490 | 606542 | CONCRETE WALL BARRIER 42" | L.F. | 1350 |  |  |
| 0500 | 607014 | WOVEN WIRE FENCE 4' | L.F. | 4500 |  |  |
| 0510 | 607015 | BRACES/CORNER POSTS | EACH | 70 |  |  |
| 0520 | 607251 | REMOVE AND RESET GATE | EACH | 3 |  |  |
| 0530 | 607308 | STANDARD GATE, 8' | EACH | 6 |  |  |
| 0540 | 607310 | STANDARD GATE, 10' | EACH | 4 |  |  |
| 0550 | 607312 | STANDARD GATE, 12' | EACH | 1 |  |  |
| 0560 | 607316 | STANDARD GATE, 16' | EACH | 4 |  |  |
| 0570 | 608006 | CONCRETE SIDEWALK 6" | S.Y. | 5 |  |  |
| 0580 | 609324 | CONCRETE SLOPED CURB AND GUTTER 6" X 24" | L.F. | 1900 |  |  |
| 0590 | 617000 | VIBRATION MONITORING | LS | 1 |  |  |
| 0600 | 618000 | TRAFFIC CONTROL MANAGEMENT | LS | 1 |  |  |
| 0610 | 618011 | PUBLIC AWARENESS | LS | 1 | $20,000.00 |  |
| 0620 | 621000 | MOBILIZATION | LS | 1 |  |  |
| 0630 | 622002 | FIELD LABORATORY, TYPE II | EACH | 1 |  |  |
| 0640 | 622100 | SUPPLEMENTAL FIELD LABORATORY | EACH | 1 |  |  |
| 0650 | 622200 | FIELD OFFICE | EACH | 1 |  |  |
| 0660 | 623324 | CURB DROP INLET TYPE IV-A, OVER 4' | EACH | 2 |  |  |
| 0670 | 623345 | CURB DROP INLET FOR CONCRETE WALL BARRIER | EACH | 10 |  |  |
| 0680 | 632000 | CLASS A SEEDING | ACRE | 9 |  |  |
| 0690 | 632020 | CLASS C SEEDING | ACRE | 3 |  |  |
| 0700 | 663049 | PRECONSTRUCTION UTILITY SURVEY | LS | 1 |  |  |
| 0710 | 663202 | GAS SYSTEM | LS | 1 | $50,000.00 |  |
| 0720 | 664000 | LANDSCAPE, COMPLETE | LS | 1 |  |  |
| 0730 | 667110 | MAIL BOX INSTALLATION-SINGLE | EACH | 3 |  |  |
| 0740 | 668000 | DEWATERING | LS | 1 |  |  |
| 0750 | 690000 | HIGHWAY/RAILWAY INTERSECTION | LS | 1 | $315,806.00 |  |
| 0760 | 690001 | RAILWAY FLAGGING | ALOW | 1 | $700,000.00 |  |
| 0770 | 701000 | PANEL SIGNS | S.F. | 200 |  |  |
| 0780 | 701100 | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS | L.F. | 420 |  |  |
| 0790 | 702610 | PORTABLE CHANGEABLE MESSAGE SIGN | EACH | 4 |  |  |
| 0800 | 702810 | TRAFFIC CONTROL DEVICES FOR CONSTRUCTION | LS | 1 |  |  |
| 0810 | 703002 | OBJECT MARKER TYPE 2 | EACH | 6 |  |  |
| 0820 | 703004 | OBJECT MARKER TYPE 4 | EACH | 25 |  |  |
| 0830 | 704700 | HOT THERMOPLASTIC PAVEMENT MARKINGS 4" | L.F. | 15800 |  |  |
| 0840 | 704704 | HOT THERMOPLASTIC PAVEMENT MARKING 24" | L.F. | 80 |  |  |
| 0850 | 801000 | CONSTRUCTION STAKING BY THE CONTRACTOR | LS | 1 |  |  |
| 0860 | 802000 | POST CONSTRUCTION PLANS | LS | 1 | $10,000.00 |  |
| 0870 | 803000 | SCHEDULE SOFTWARE | LS | 1 |  |  |
| 0880 | 803010 | CPM TRAINING | LS | 1 |  |  |
| 0890 | 803020 | CPM HARDWARE/EQUIPMENT | LS | 1 |  |  |

Date Generated

**Mar 20, 2023**

Call Order

**002**

Project ID

**4101400**

Amendments

**0**

Counties

**Quay**

Highway Number

Time Remaining

Add to calendar

Days

**24**

Hours

**3**

Description

**Roadway Rehabilitation, Bridge Rehabilitation**

Items

Favorite items only

Edit favorites

Export

| **Line** | **Item** | **Description** | **Unit** | **Quantity** | **Price** | |
| --- | --- | --- | --- | --- | --- | --- |
| Section 0001: ROADWAY | | | | | | |
| 0010 | 203000 | UNCLASSIFIED EXCAVATION | C.Y. | 896 |  |  |
| 0020 | 203200 | UNSUITABLE MATERIAL EXCAVATION | C.Y. | 14019 |  |  |
| 0030 | 203211 | UNSTABLE SUBGRADE STABILIZATION | S.Y. | 21029 |  |  |
| 0040 | 207000 | SUBGRADE PREPARATION | S.Y. | 334 |  |  |
| 0050 | 209000 | BLADING AND RESHAPING | MILE | 10 |  |  |
| 0060 | 403705 | WARM MIX OPEN-GRADED FRICTION COURSE COMPLETE | TON | 4151 |  |  |
| 0070 | 407000 | ASPHALT MATERIAL FOR TACK COAT | TON | 146 |  |  |
| 0080 | 408100 | PRIME COAT MATERIAL | TON | 49 |  |  |
| 0090 | 414000 | COLD MILLING (ASPHALT) | SYIN | 1169066 |  |  |
| 0100 | 416113 | MINOR PAVING TYPE I, WMA SP-III | TON | 5792 |  |  |
| 0110 | 416213 | MINOR PAVING TYPE II, WMA SP-III | TON | 93 |  |  |
| 0120 | 424003 | WMA SP-III COMPLETE | TON | 49823 |  |  |
| 0130 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| 0140 | 601110 | REMOVAL OF SURFACING | S.Y. | 3756 |  |  |
| 0150 | 603262 | COMPOSTED MULCH SOCKS | L.F. | 1450 |  |  |
| 0160 | 603281 | SWPPP PLAN PREPARATION AND MAINTENANCE | LS | 1 |  |  |
| 0170 | 605000 | UNDERDRAINS | L.F. | 6800 |  |  |
| 0180 | 606001 | SINGLE FACE W-BEAM GUARDRAIL | L.F. | 14775 |  |  |
| 0190 | 606051 | END TREATMENT TL-3 END TERMINAL | EACH | 13 |  |  |
| 0200 | 606053 | END TREATMENT W-BEAM END ANCHOR | EACH | 13 |  |  |
| 0210 | 606061 | DRAINAGE STRUCTURE PROTECTION SYSTEM | L.F. | 50 |  |  |
| 0220 | 606062 | TRANSITION METAL BARRIER TO RIGID BARRIER | EACH | 8 |  |  |
| 0230 | 606498 | POST AND CABLE BARRIER END ANCHOR | EACH | 4 |  |  |
| 0240 | 606499 | POST AND CABLE BARRIER | L.F. | 1000 |  |  |
| 0250 | 606598 | TCWB RETAINED BY THE CONTRACTOR | L.F. | 5740 |  |  |
| 0260 | 606599 | RESETTING OF TCWB | L.F. | 6340 |  |  |
| 0270 | 618000 | TRAFFIC CONTROL MANAGEMENT | LS | 1 |  |  |
| 0280 | 618011 | PUBLIC AWARENESS | LS | 1 | $5,000.00 |  |
| 0290 | 621000 | MOBILIZATION | LS | 1 |  |  |
| 0300 | 622300 | FIELD LABORATORY TESTING EQUIPMENT | LS | 1 | $280,000.00 |  |
| 0310 | 631000 | RUMBLE STRIPS | L.F. | 105437 |  |  |
| 0320 | 701000 | PANEL SIGNS | S.F. | 817 |  |  |
| 0330 | 701100 | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS | L.F. | 1850 |  |  |
| 0340 | 701101 | MULTI-DIRECTIONAL SLIP BASE POSTS FOR ALUMINUM PANEL SIGNS | EACH | 2 |  |  |
| 0350 | 702000 | CONSTRUCTION SIGNING | S.F. | 196 |  |  |
| 0360 | 702100 | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING | L.F. | 174 |  |  |
| 0370 | 702101 | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING | EACH | 12 |  |  |
| 0380 | 702610 | PORTABLE CHANGEABLE MESSAGE SIGN | EACH | 4 |  |  |
| 0390 | 702810 | TRAFFIC CONTROL DEVICES FOR CONSTRUCTION | LS | 1 |  |  |
| 0400 | 702850 | LAW ENFORCEMENT IN CONSTRUCTION ZONE | ALOW | 1 | $20,000.00 |  |
| 0410 | 703100 | ROAD DELINEATOR TYPE GUIDE | EACH | 90 |  |  |
| 0420 | 703400 | 1/10TH MILE DELINEATOR | EACH | 90 |  |  |
| 0430 | 704002 | RETROREFLECTORIZED PAINTED MARKINGS 6" | L.F. | 239321 |  |  |
| 0440 | 704004 | RETROREFLECTORIZED PAINTED MARKINGS 12" | L.F. | 7200 |  |  |
| 0450 | 704869 | PLOWABLE REFLECTIVE RAISED PAVEMENT MARKER TYPE PG | EACH | 38 |  |  |
| 0460 | 704872 | PLOWABLE REFLECTIVE RAISED PAVEMENT MARKER TYPE PC | EACH | 1318 |  |  |
| 0470 | 704876 | TEMPORARY REFLECTIVE RAISED PAVEMENT MARKER, TYPE TG | EACH | 3954 |  |  |
| 0480 | 720060 | VEHICULAR IMPACT ATTENUATOR UNIT-WORK ZONES | EACH | 3 |  |  |
| 0490 | 720110 | REMOVE/RESET IMPACT ATTENUATOR UNIT | EACH | 3 |  |  |
| 0500 | 801000 | CONSTRUCTION STAKING BY THE CONTRACTOR | LS | 1 |  |  |
| 0510 | 802000 | POST CONSTRUCTION PLANS | LS | 1 | $2,500.00 |  |
| Section 0002: BRIDGE | | | | | | |
| 0520 | 511070 | STRUCTURAL CONCRETE, CLASS HPD | C.Y. | 38 |  |  |
| 0530 | 515000 | REINF.CONCRETE FOR MINOR STRUCTURES | C.Y. | 8 |  |  |
| 0540 | 533000 | REPAIR OF CONCRETE STRUCTURES | S.Y. | 40 |  |  |
| 0550 | 540160 | EPOXY COATED REINFORCING BARS GRADE 60 | LB | 4800 |  |  |
| 0560 | 548002 | COATING OF CONCRETE - PAINT | S.F. | 600 |  |  |
| 0570 | 563099 | POLYMER BRIDGE JOINT SEALS | L.F. | 14 |  |  |
| 0580 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| 0590 | 602000 | RIPRAP CLASS A | C.Y. | 40 |  |  |
| 0600 | 602060 | RIPRAP CLASS G | S.Y. | 60 |  |  |

Date Generated

**Mar 20, 2023**

Call Order

**003**

Project ID

**6101231**

Amendments

**0**

Counties

**Sandoval**

Highway Number

Time Remaining

Add to calendar

Days

**24**

Hours

**3**

Description

**Roadway Reconstruction**

Items

Favorite items only

Edit favorites

Export

| **Line** | **Item** | **Description** | **Unit** | **Quantity** | **Price** | |
| --- | --- | --- | --- | --- | --- | --- |
| Section 0001: ROADWAY | | | | | | |
| 0010 | 201000 | CLEARING AND GRUBBING | LS | 1 |  |  |
| 0020 | 203000 | UNCLASSIFIED EXCAVATION | C.Y. | 2700 |  |  |
| 0030 | 203100 | BORROW | C.Y. | 400 |  |  |
| 0040 | 203211 | UNSTABLE SUBGRADE STABILIZATION | S.Y. | 800 |  |  |
| 0050 | 207000 | SUBGRADE PREPARATION | S.Y. | 3000 |  |  |
| 0060 | 207051 | SOIL MIXING | C.Y. | 4630 |  |  |
| 0070 | 303000 | BASE COURSE | TON | 1200 |  |  |
| 0080 | 405000 | DETOUR PAVEMENT CONSTRUCTION | S.Y. | 990 |  |  |
| 0090 | 407000 | ASPHALT MATERIAL FOR TACK COAT | TON | 2 |  |  |
| 0100 | 408100 | PRIME COAT MATERIAL | TON | 7 |  |  |
| 0110 | 416103 | MINOR PAVING TYPE I, HMA SP-III | TON | 950 |  |  |
| 0120 | 515000 | REINF.CONCRETE FOR MINOR STRUCTURES | C.Y. | 6 |  |  |
| 0130 | 516000 | FLOWABLE FILL | C.Y. | 16 |  |  |
| 0140 | 570024 | 24" CULVERT PIPE | L.F. | 4 |  |  |
| 0150 | 601000 | REMOVAL OF STRUCTURES AND OBSTRUCTIONS | LS | 1 |  |  |
| 0160 | 601110 | REMOVAL OF SURFACING | S.Y. | 3000 |  |  |
| 0170 | 603100 | TEMPORARY SOIL STABILANT | ACRE | 2.4 |  |  |
| 0180 | 603250 | DROP INLET PROTECTION TYPE I | EACH | 1 |  |  |
| 0190 | 603262 | COMPOSTED MULCH SOCKS | L.F. | 30 |  |  |
| 0200 | 603281 | SWPPP PLAN PREPARATION AND MAINTENANCE | LS | 1 |  |  |
| 0210 | 604100 | IMPERMEABLE MEMBRANE LINER | S.Y. | 430 |  |  |
| 0220 | 606001 | SINGLE FACE W-BEAM GUARDRAIL | L.F. | 575 |  |  |
| 0230 | 606052 | END TREATMENT TL-2 END TERMINAL | EACH | 1 |  |  |
| 0240 | 606063 | EXISTING BEAM GUARDRAIL TO 31" BEAM GUARDRAIL TRANSITION | EACH | 1 |  |  |
| 0250 | 606598 | TCWB RETAINED BY THE CONTRACTOR | L.F. | 880 |  |  |
| 0260 | 606599 | RESETTING OF TCWB | L.F. | 880 |  |  |
| 0270 | 607004 | BARBED WIRE FENCE 4' | L.F. | 1700 |  |  |
| 0280 | 607015 | BRACES/CORNER POSTS | EACH | 12 |  |  |
| 0290 | 610000 | CATTLE GUARD | L.F. | 36 |  |  |
| 0300 | 618000 | TRAFFIC CONTROL MANAGEMENT | LS | 1 |  |  |
| 0310 | 618011 | PUBLIC AWARENESS | LS | 1 | $5,000.00 |  |
| 0320 | 621000 | MOBILIZATION | LS | 1 |  |  |
| 0330 | 622001 | FIELD LABORATORY, TYPE I | EACH | 1 |  |  |
| 0340 | 622110 | SUPPLEMENTAL HOT-MIX ASPHALT FIELD LABORATORY | EACH | 1 |  |  |
| 0350 | 623059 | MODIFIED MEDIAN DROP INLET TYPE II (VALLEY/URBAN) | EACH | 1 |  |  |
| 0360 | 632000 | CLASS A SEEDING | ACRE | 1 |  |  |
| 0370 | 632020 | CLASS C SEEDING | ACRE | 1 |  |  |
| 0380 | 701000 | PANEL SIGNS | S.F. | 45 |  |  |
| 0390 | 701100 | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS | L.F. | 60 |  |  |
| 0400 | 702000 | CONSTRUCTION SIGNING | S.F. | 41 |  |  |
| 0410 | 702100 | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING | L.F. | 50 |  |  |
| 0420 | 702610 | PORTABLE CHANGEABLE MESSAGE SIGN | EACH | 2 |  |  |
| 0430 | 702612 | PORTABLE FLOODLIGHT SYSTEM | EACH | 2 |  |  |
| 0440 | 702710 | MOBILE TRAFFIC SIGNAL SYSTEM | EACH | 1 |  |  |
| 0450 | 702810 | TRAFFIC CONTROL DEVICES FOR CONSTRUCTION | LS | 1 |  |  |
| 0460 | 703100 | ROAD DELINEATOR TYPE GUIDE | EACH | 2 |  |  |
| 0470 | 704000 | RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 7300 |  |  |
| 0480 | 704099 | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" | L.F. | 4100 |  |  |
| 0490 | 720060 | VEHICULAR IMPACT ATTENUATOR UNIT-WORK ZONES | EACH | 2 |  |  |
| 0500 | 720110 | REMOVE/RESET IMPACT ATTENUATOR UNIT | EACH | 2 |  |  |
| 0510 | 721000 | REMOVAL OF PAVEMENT MARKING | L.F. | 4100 |  |  |
| 0520 | 801000 | CONSTRUCTION STAKING BY THE CONTRACTOR | LS | 1 |  |  |
| 0530 | 802000 | POST CONSTRUCTION PLANS | LS | 1 | $5,000.00 |  |
| 0540 | 803000 | SCHEDULE SOFTWARE | LS | 1 |  |  |
| 0550 | 803020 | CPM HARDWARE/EQUIPMENT | LS | 1 |  |  |